                            7-01 VERSION DATE:  980601

                Chapter 7 - Data Return

                         Contents

                         ________

       Sub-Section                                      Page

7.0    Contents  .....................................    1

7.1    Introduction to Chapter 7  ....................    2

7.2    NIMS IFL Observation Geometry Plot  ...........    3

7.3    NIMS Archived EDRs and CUBEs  .................    4

7.4    NIMS Data Formats, Types, Labels and Access  ..   5-6

7.5    Understanding the NIMS Mask  ..................    7

                                 7-02

                       Introduction to Chapter 7

     This chapter is a report on the NIMS data return for the
In-Flight Load (IFL).  The IFL was the time period between J0
and G1 when the NIMS phase2 RAM software was first loaded from
the ground and tested.

     After the phase2 software was loaded, three OPCAL sequences
were performed and returned in realtime.  These OPCALs were used
to verify that the software had loaded properly and to also test
the new phase2 capabilities, such as real-time data return,
wavelength editing and mirror blocking.

     The new Galileo Ground Data System (GDS) and AMMOS were also
tested in preparation for Orbital Operations as well as the MIPS
real time data processing.  This tested the entire ground path
from DSN Station to UDR to Tube.

     The plot on the page 3 shows the geometry of the NIMS IFL
observations using a north trajectory pole projection.

     The text on pages 4 gives a brief discussion of the NIMS data
files.  Additional information about NIMS data formats, data types,
data labels and data access is given on pages 5 and 6.

     The text on page 7 is a guide to understanding the NIMS MASK.

                            7-03

                                          NIMS - FEL - 10/16/98

   NIMS IN-FLIGHT LOAD (IFL)

     G1 North Trajectory Pole View, Apoapsis to Apoapsis

Ganymede Flyby (G1): 27-JUN-1996 (D179) 06:29:05 UTC
     Perijove (PJ1): 28-JUN-1996 (D180) 00:31:24 UTC

Time Ticks (Relative to G1)
Spacecraft - 2 Days

                                                                            IFLIFL RAM LOAD

                                                                            IFLNIMSOCAL1

                                                                            IFLNIMSOCAL2

                                                                            IFLNIMSOCAL3

                                                                            CHOPPER OFF

                                                                            D177

                                                                            D189

                                                                            PJ1G1ESAPO-1

                                                                            APO-2

                                 7-04

NIMS Archived EDRs and CUBEs

____________________________

     The NIMS data are stored in EDRs (Experimental Data Records)
produced by JPL-MIPS (Multi-mission Image Processing System).
The NIMS Phase2 EDR is described in the NIMS EDR SIS (Software
Interface Specification) Number 232-08.  The same information
is available in both human and machine-readable form in the PDS
(Planetary Data System) structure files EDRHDR.FMT and EDRDATA.FMT
in the LABEL directory of the NIMS EDR CD-ROM.  Each observation
has at least one EDR.  The EDR file name is derived from the 12
character observation name plus a single character which allows
an observation to be broken up into multiple EDRs.  The EDRs have
a Vicar label, followed by a PDS/ISIS label, binary header records
and the data records.  For archiving on CD-ROM, the Vicar labels
are detached from the EDR (but kept separately on CD) and the file
is renamed so as to conform to the 8.3 DOS file-naming convention.
The 8.3 EDR name consists of a 2 character orbit identifier, a
single character target identifier, a 3 digit counter and the
suffix EDR.  For example, the MIPS EDR G1GNGLOBAL01A.1 becomes
G1G001.EDR.  More information about NIMS EDRs can be found in the
VOLINFO.TXT file on the EDR CD-ROM.

     NIMS EDR data typically require considerable processing before
they are readily amenable to science analysis.  Normally, the EDRs
are processed into spectral image cubes by one of several sets of
software.  MIPS systematically processes the EDRs into CUBEs (band
sequential image files) and MASKs (spatial/spectral summary images)
which are distributed on the NIMS CUBE CD-ROMs.  Information about
the structure of the NIMS CUBEs can be found in the VOLINFO.TXT file
on the CUBE CD-ROM.  The name of the CUBE file is derived from the
input EDR filename.  For archiving on CD-ROM, the CUBE files are
renamed so as to conform to the 8.3 DOS file-naming convention.  The
8.3 CUBE name consists of a 2 character orbit identifier, a single
character target identifier, a 3 digit counter, a single character
cube-type identifier, a single character data unit-type (DN, radiance
or IOF) and the suffix QUB.  For example, the MIPS IOF radiance cube
for the observation G1GNGLOBAL01A.1 (G1G001) becomes G1G001CR.EDR.
The summary MASKs on the CD-ROM have the same 6 character name as the
EDR name with the suffix JPG or GIF to denote its graphics format.

                                 7-05

NIMS Data Format - Data types - Data Labels - Data Access

_________________________________________________________

Data Format

___________

All data files have PDS labels.  The raw data (EDR) file contains
time-sequential, 16 bit integers.  Reduced data files (TUBES and
CUBES) may be viewed as images or spectra.  They contain VAX real
numbers, are band sequential (BSQ - the images are stacked in band
order) and have geometry information appended as backplanes after
the last NIMS band.

Data Types

__________

Mask files contain summary images (3 band BSQ) and spectra of up to
six selected regions that provide a quick indication of data location,
data quality and spectral content.  A Guide to understanding the NIMS
mask is available.

Cube files contain data that have been projected and resampled.  The
core data are BSQ - spatial in the first two dimensions, and spectral
in the third. Cubes of the satellites are projected in point-of-view,
and, with few exceptions have no photometric correction applied.
Cubes of Jupiter are (generally) projected as simple cylindrical.
Cubes of Europa, Ganymede, and Callisto have been despiked. The cubes
are available both in radiance and I/F (intensity divided by flux)
form.

Tube files contain data in (almost) time order and normally have
a NIMS-related 20 pixel spatial dimension (20 x n or n x 20).
Projection coordinates are contained in backplanes, but the data
have not been resampled.  The data are in units of radiance and no
despiking has been applied.  All data in cubes are also available in
tube form. Some data (such as spatially undersampled data) appear in
tube form only.

A spike file contains a list of pixels that have been identified as
spikes, but not replaced, in the tube. Spike files can be used to
remove spikes from both tube and EDR files.

EDR files contain the most primitive form of the data available.
They should be used only for advanced data analysis.  The format is
complex and the files do not form images or spectra without prior
processing.

                                 7-06

NIMS Data Format - Data types - Data Labels - Data Access

_________________________________________________________

Data Labels

___________

A data label (PDS form) is attached to the front of each file (except
masks, which have an attached VICAR label and a detached PDS label).
The labels are in ASCII keyword=value format and contain pointers to
various data objects in the file, descriptions of the data objects and
descriptions of the observation associated with the file.  A history
object in similar format follows and describes the processing steps
that produced the file.  Much of this information is necessary for
understanding and viewing the cube.  In particular, the label contains
the offset to the cube, the dimensions of the cube, axes labels, and
explicit wavelength information.

Data Access

___________

Software for processing this data is called ISIS and is available for
DEC VAX VMS, SUN Solaris, DEC Alpha Digital Unix, Silicon Graphics
Unix and PC LINUX systems.  The Unix versions are available from the
USGS Astrogeology team.  Images from NIMS cubes and tubes can be
viewed with any image display program which allows an offset from the
beginning of the file to the selected image.  Packages tested include
ISIS, VICAR, ENVI, SAO IMAGE, and NASAVIEW. ISIS and ENVI (and soon
NASAVIEW) additionally display spectra.  The ISIS viewer is named CV
(UNIX) or QL3 (VMS).

Labels may be displayed with some editors (eg DOS edit), and with most
"type" and "search" functions. Some editors do not recognize the PDS
line termination conventions. The label may be listed by the ISIS
function LHLIST (VMS) or LABEL (UNIX).

Software for converting EDRs to cubes exist in both ISIS (DEC VAX VMS)
and VICAR (DEC Alpha VMS) versions only.  A primitive list of values
in an EDR may be obtained with the program EDRDMP2.

                                 7-07

Understanding the NIMS Mask

___________________________

     The NIMS mask is designed to provide a quick summary of the
contents of a NIMS data cube (or tube).  It displays a view of both
the spatial and spectral content of the data.

     The mask has four regions.  Starting from the upper left and
proceeding clockwise:  a spatial display; six or fewer representative
spectra; annotation; and a spectral histogram.

     The spatial display of an observation which has been projected
and resampled (a cube) has a maximum size of 600x600 pixels.  This
is overlaid with surface coordinates and is embedded in a 700x700
grid of pixel coordinates.  It is accompanied by two 1-dimensional
histograms describing the raw image and the image stretched for
display.  The data image can range from a simple combination of up to
3 NIMS bands displayed in the RGB planes, to complicated arithmetic
functions of NIMS bands displayed in the RGB planes.  (The formulas
appear as annotation below the histograms.)  The graphics directly
below the image show the input and output data histograms for the
three color planes. The "shortest" color for each bin displays in
front.  The image also contains from one to six numbered rectangles,
which show the from which averaged spectra (displayed on the right)
were taken.

     The spatial display of an observation in time sequence (a tube)
is a graphic showing a footprint of the observation over a grid of
surface coordinates on the target body.  Numerals 1-6 on the graphic
mark the locations of the average spectra displayed on the right.

     The spectra to the right of the image may display either BDRF or
radiance (or both).  If both are displayed, then a vertical "radiance
fence" line will appear where the breakpoint occurs.  This permits
display of both atmospheric data, which have significant reflectance
and thermal components, and I/F satellite surface data which have
strong absorptions at longer wavelengths (such as water spectra.)
The spectra are labelled with wavelength in microns and location in
both pixel and latitude-longitude space.

     The annotation provides information about the observation,
including its name, a brief description, its geometry, instrument and
projection parameters.  TCA is the time from Galileo’s closest
approach to the target body.

     The 2-dimensional spectral histogram in the lower left corner
shows the number of pixels at a given radiance for each wavelength.
If a surface contains spatial mixtures with significantly different
spatial fractions for several components, the spectra of the
components will be evident in this display.