Fig. 13. Parameter Table Assignments.

Spectral modes are derived from the number of grating positions N, the increment between successive grating positions D, and the starting position of the grating, S. Spatial scanning is controlled by the mirror operation bit, M.