PDS4 Local Data Dictionary Processing Report

Configuration:
   LDDTool Version        15.3.0
   LDD Version Id:        1.0.2.0
   LDD Label Version Id:  1.27
   LDD Discipline (T/F):  false
   LDD Namespace URL:     http://www.kari.re.kr/kpds/
   LDD URN Prefix:        urn:kari:kpds:
   Time                   Wed Sep 24 19:06:19 UTC 2025
   Common Schema          [PDS4_PDS_1L00.xsd]
   Common Schematron      [PDS4_PDS_1L00.sch]
   IM Version Id:         1.21.0.0
   IM Namespace Id:       pds
   IM Label Version Id:   1.27
   IM Object Model        [UpperModel.pont]
   IM Data Dictionary     [dd11179.pins]
   IM Glossary            [Glossary.pins]
   IM Document Spec       [DMDocument.pins]

Parameters:
   Input File             [/home/runner/work/ldd-kplo/ldd-kplo/src/PDS4_KPLO_IngestLDD.xml]
   PDS Processing         true
   LDD Processing         true
   Discipline LDD         false
   Mission LDD            true
   Write Attr Elements    false
   Merge with Master      false

Summary:
   Classes                3
   Attributes             81
   Associations           85
   Error messages         0
   Warning messages       0
   Information messages   0

Detailed validation messages

Parsed Input - Header:
   LDD Name               KPLO
   LDD Version            1.0.2.0
   Full Name              Trent Hare
   Steward                img
   Namespace Id           kplo
   Comment                
        The KPLO dictionary contains classes that describe aspects of the 
        Korea Pathfinder Lunar Orbiter mission and related instruments.
    
   Last Modification Time 2025-09-22T12:00Z
   PDS4 Merge Flag        false

Parsed Input - Attributes:

   name                   bias_spread
   version                1.21
   value data type        ASCII_Integer
   description            Difference between the max and min bias 12-bit DN value for the whole image.

   name                   bias_spread_ch0
   version                1.21
   value data type        ASCII_Integer
   description            Difference between the max and min bias 12-bit DN value for channel 0.

   name                   bias_spread_ch1
   version                1.21
   value data type        ASCII_Integer
   description            Difference between the max and min bias 12-bit DN value for channel 1.

   name                   bias_spread_ch2
   version                1.21
   value data type        ASCII_Integer
   description            Difference between the max and min bias 12-bit DN value for channel 2.

   name                   bias_spread_ch3
   version                1.21
   value data type        ASCII_Integer
   description            Difference between the max and min bias 12-bit DN value for channel 3.

   name                   bias_spread_ch4
   version                1.21
   value data type        ASCII_Integer
   description            Difference between the max and min bias 12-bit DN value for channel 4.

   name                   bias_spread_ch5
   version                1.21
   value data type        ASCII_Integer
   description            Difference between the max and min bias 12-bit DN value for channel 5.

   name                   bit_selection
   version                1.21
   value data type        ASCII_Integer
   description            The ADC bit selection is for the used bit range flag. The value 0 is for bit range 11 ~ 0 and detectable range 0~4095, the value 1 is for bit range 12 ~ 1 and detectable range 0~8190, and the value 2 is for bit range 13 ~ 2 and detectable range 0~16380. 

   name                   bterm1
   version                1.21
   value data type        ASCII_Integer
   description            ShadowCam companding bterm 1 (See appendix in the ShadowCam archive SIS for detailed companding information)

   name                   bterm2
   version                1.21
   value data type        ASCII_Integer
   description            ShadowCam companding bterm 2 (See appendix in the ShadowCam archive SIS for detailed companding information)

   name                   bterm3
   version                1.21
   value data type        ASCII_Integer
   description            ShadowCam companding bterm 3 (See appendix in the ShadowCam archive SIS for detailed companding information)

   name                   bterm4
   version                1.21
   value data type        ASCII_Integer
   description            ShadowCam companding bterm 4 (See appendix in the ShadowCam archive SIS for detailed companding information)

   name                   bterm5
   version                1.21
   value data type        ASCII_Integer
   description            ShadowCam companding bterm 5 (See appendix in the ShadowCam archive SIS for detailed companding information)

   name                   ccd_direction
   version                1.21
   value data type        ASCII_Integer
   description             The CCD direction parameter defines the direction of CCD reading. The value 0 is for the reading direction from 1st pixel to 2048th pixel (default) and the value 1 is from the reading direction from 2048th pixel to 1st pixel. 

   name                   compression_mode
   version                1.21
   value data type        ASCII_Integer
   description            compression_mode is set by ground command. Default value is 1 for compression on and 0 for off.

   name                   compression_ratio
   version                1.21
   value data type        ASCII_Integer
   description            compression_ratio is set by ground command. Default value is 0 for losses. Range is from 0 to 255
   minimum value          0
   maximum value          255

   name                   constant_offset_data
   version                1.21
   value data type        ASCII_Integer
   description            constant_offset is set by ground command. Default value is 0. if prescan mode is 2, then this value will be used.

   name                   data_quality_desc
   version                1.21
   value data type        ASCII_Text_Collapsed
   description             Describes how to interpret the data_quality_id field. 

   name                   data_quality_id
   version                1.21
   value data type        ASCII_Short_String_Collapsed
   description             LROC-style data quality ID bitmask with minimal differences between ShadowCam and LROC definitions. See data_quality_desc for details. The individual boolean fields (dqi_*) are likely easier to use for new software. 

   name                   dqi_corruption_detected
   version                1.21
   value data type        ASCII_Boolean
   description             The corruption detection algorithm found a strong likelihood of image corruption somewhere in the observation. This is often localized to a small area, leaving most of the image usable. 

   name                   dqi_fpa_out_of_bounds
   version                1.21
   value data type        ASCII_Boolean
   description             The focal plane temperature was outside of the nominal operational limits. The calibration of the image is likely to not be as good in this case. 

   name                   dqi_missing_data
   version                1.21
   value data type        ASCII_Boolean
   description             One or more 1 MiB data blocks are missing from the image. Due to interleaving, this typically results in a pattern of 4 pixels present 4 pixels missing. 

   name                   dqi_missing_spice
   version                1.21
   value data type        ASCII_Boolean
   description             SPICE was unavailable for this observation. 

   name                   dqi_uncalibratable
   version                1.21
   value data type        ASCII_Boolean
   description             This observation could not be calibrated. 

   name                   dqi_under_saturated
   version                1.21
   value data type        ASCII_Boolean
   description             One or more 0 DN values are present in the companded 8-bit DN. 

   name                   execution_spacecraft_time
   version                1.21
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft time of when the image command was executed. Use this time with the SCLK kernel and add the start_time_offset value for the most accurate image start. 

   name                   execution_time
   version                1.21
   value data type        ASCII_Date_Time_YMD
   description            The UTC time and date at the execution of the image acquisition command. Add the start time offset to this time to get the start of the image data. Use the spacecraft clock version of the time with an SCLK kernel for the most accurate timing. 

   name                   frame_id
   version                1.21
   value data type        ASCII_Short_String_Collapsed
   description            Records if the image was LUTI A or B

   name                   gain_ch0
   version                1.21
   value data type        ASCII_Integer
   description             The analog front end gain for channel 0. See ShadowCam calibration paper for details on the gain correction. 

   name                   gain_ch1
   version                1.21
   value data type        ASCII_Integer
   description             The analog front end gain for channel 1. See ShadowCam calibration paper for details on the gain correction. 

   name                   gain_ch2
   version                1.21
   value data type        ASCII_Integer
   description             The analog front end gain for channel 2. See ShadowCam calibration paper for details on the gain correction. 

   name                   gain_ch3
   version                1.21
   value data type        ASCII_Integer
   description             The analog front end gain for channel 3. See ShadowCam calibration paper for details on the gain correction. 

   name                   gain_ch4
   version                1.21
   value data type        ASCII_Integer
   description             The analog front end gain for channel 4. See ShadowCam calibration paper for details on the gain correction. 

   name                   gain_ch5
   version                1.21
   value data type        ASCII_Integer
   description             The analog front end gain for channel 4. See ShadowCam calibration paper for details on the gain correction. 

   name                   klines
   version                1.21
   value data type        ASCII_Integer
   description             The number of 1024-line image chunks commanded (includes preroll). 

   name                   line_rate
   version                1.21
   value data type        ASCII_Real
   description            line time in hertz
   unit of measure type   Units_of_Frequency

   name                   line_time
   version                1.21
   value data type        ASCII_Real
   description            line time in milliseconds
   unit of measure type   Units_of_Time

   name                   line_integration_time
   version                1.21
   value data type        ASCII_Real
   description             The line integration time in milliseconds. 
   unit of measure type   Units_of_Time

   name                   line_rate_code
   version                1.21
   value data type        ASCII_Integer
   description             The TDI line rate code commanded. The line time in seconds can be computed from the commanded line rate using the expression 50e-9*(12*524+(lr*(38+1)+46)), where lr is thecommanded line rate (0-4095). 

   name                   line_rate_ms
   version                1.21
   value data type        ASCII_Real
   description             The TDI line rate in milliseconds, the effective exposure time is multiplied by 32 for the number of TDI stages. 
   unit of measure type   Units_of_Time

   name                   luti_constant_time_offset
   version                1.21
   value data type        ASCII_Real
   description             Constant time offset for LUTI A or B in seconds. 
   unit of measure type   Units_of_Time

   name                   luti_quality_id
   version                1.21
   value data type        ASCII_Integer
   description             For LUTI, the quality ID represents the error status of the image. 0: No error, 1: CRC error, 2: CRC error + compression/decompression error. 

   name                   luti_target_type
   version                1.21
   value data type        ASCII_Short_String_Collapsed
   description             The luti target type is for LUTI target type such as MLND (Lunar surface, moon landing candidates), MMMO (man made objects), MCRT (lunar craters), MPIT (lunar pits), CGEO (calibration target for geocal), CDRK (dark), CLIM(lunar limb), LSLT (side slither), CSTA (star image), SERT (special targets for the earth), SPLT (planets), and SMS1 and SMS2 (special lunar surface image). 

   name                   luti_target_name
   version                1.21
   value data type        ASCII_Short_String_Collapsed
   description             The luti target name indicates the name of target areas if it is available. If it is not, it will show NA. 

   name                   mission_phase_name
   version                1.21
   value data type        ASCII_Short_String_Collapsed
   description             The mission_phase_name attribute provides the mission-defined name of a time period within the mission. 

   name                   mode_test
   version                1.21
   value data type        ASCII_Boolean
   description             The instrument was commanded in test mode, resulting in a gradient rather than image data. 

   name                   offset_ch0
   version                1.21
   value data type        ASCII_Integer
   description             The analog front end offset for channel 0. 

   name                   offset_ch1
   version                1.21
   value data type        ASCII_Integer
   description             The analog front end offset for channel 1. 

   name                   offset_ch2
   version                1.21
   value data type        ASCII_Integer
   description             The analog front end offset for channel 2. 

   name                   offset_ch3
   version                1.21
   value data type        ASCII_Integer
   description             The analog front end offset for channel 3. 

   name                   offset_ch4
   version                1.21
   value data type        ASCII_Integer
   description             The analog front end offset for channel 4. 

   name                   offset_ch5
   version                1.21
   value data type        ASCII_Integer
   description             The analog front end offset for channel 5. 

   name                   orbit_number
   version                1.21
   value data type        ASCII_Integer
   description            The orbit_number attribute identifies the number of the orbital revolution of the spacecraft around the Moon. 
   nillable               true
   minimum value          0

   name                   pre_scan_mode_selection
   version                1.21
   value data type        ASCII_Integer
   description             The pre scan mode selection flag is set by ground command. Default value is 1. The value 0 is for disable of use of pre-scan pixel and the value 1 is to use averaged value of pre-scan pixel and the value 2 is to use constant offset value predefined. 

   name                   preroll_lines
   version                1.21
   value data type        ASCII_Integer
   description             The number of image lines dropped to initialize the TDI sensor. Typically, this is a minimum of 256. 

   name                   preroll_time
   version                1.21
   value data type        ASCII_Date_Time_YMD
   description            The UTC time and date at the start of the image acquisition, corresponding to the acquisition of preroll_lines at the given exposure prior to the actual image acquisition. 

   name                   producer_institution_name
   version                1.21
   value data type        ASCII_Short_String_Preserved
   description            The producer_institution_name attribute identifies a university, research center, NASA center, or other institution associated with the production of a data product. 

   name                   product_version_id
   version                1.21
   value data type        ASCII_Short_String_Collapsed
   description             A version specifier to differentiate how the data was processed. 

   name                   rationale_desc
   version                1.21
   value data type        ASCII_Text_Preserved
   description             Any available commentary on the goal of the observation. This is created at planning time, and specific instrument and spacecraft performance may impact if the resulting image meets the original goal or not. 

   name                   spacecraft_clock_start_count
   version                1.21
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_start_count attribute provides the value of the spacecraft clock at the beginning of a time period of interest. 

   name                   spacecraft_clock_stop_count
   version                1.21
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_stop_count attribute provides the value of the spacecraft clock at the beginning of a time period of interest. 

   name                   start_time_offset
   version                1.21
   value data type        ASCII_Real
   description             The time in seconds after the execution time that the first image row started. Use this with execution_spacecraft_time and the KPLO SCLK kernel to get the best available start of the image data. 
   unit of measure type   Units_of_Time

   name                   tdi_direction
   version                1.21
   value data type        ASCII_Short_String_Collapsed
   description             The TDI direction of the sensor (A or B). This must match the flight direction of the spacecraft except for calibration images. 

   name                   temperature_case_start
   version                1.21
   value data type        ASCII_Real
   description            The case temperature is recorded at the beginning of the line
   unit of measure type   Units_of_Temperature

   name                   temperature_case_end
   version                1.21
   value data type        ASCII_Real
   description            The case temperature is recorded at the end of the line
   unit of measure type   Units_of_Temperature

   name                   temperature_ccd_start
   version                1.21
   value data type        ASCII_Real
   description            The ccd temperature is recorded at the beginning of the line
   unit of measure type   Units_of_Temperature

   name                   temperature_ccd_end
   version                1.21
   value data type        ASCII_Real
   description            The ccd temperature is recorded at the end of the line
   unit of measure type   Units_of_Temperature

   name                   temperature_fpe_start
   version                1.21
   value data type        ASCII_Real
   description            The fpe temperature is recorded at the beginning of the line
   unit of measure type   Units_of_Temperature

   name                   temperature_fpe_end
   version                1.21
   value data type        ASCII_Real
   description            The fpe temperature is recorded at the end of the line
   unit of measure type   Units_of_Temperature

   name                   temperature_psu_start
   version                1.21
   value data type        ASCII_Real
   description            The psu temperature is recorded at the beginning of the line
   unit of measure type   Units_of_Temperature

   name                   temperature_psu_end
   version                1.21
   value data type        ASCII_Real
   description            The psu temperature is recorded at the end of the line
   unit of measure type   Units_of_Temperature

   name                   temperature_fpa_a
   version                1.21
   value data type        ASCII_Real
   description             The temperature of the ‘A’ sensor adjacent to the focal plane. This sensor is located on the heat strap going to the radiator and is the primary temperature used for calibration. 
   unit of measure type   Units_of_Temperature

   name                   temperature_fpa_b
   version                1.21
   value data type        ASCII_Real
   description             The temperature of the ‘B’ sensor adjacent to the focal plane. This sensor is on the opposite side of the TDI sensor from ‘A’, but is not on the copper strap. 
   unit of measure type   Units_of_Temperature

   name                   temperature_fpga
   version                1.21
   value data type        ASCII_Real
   description             The temperature reported on the electronics board adjacent to the FPGA. 
   unit of measure type   Units_of_Temperature

   name                   temperature_telescope
   version                1.21
   value data type        ASCII_Real
   description             The temperature reported from the metering structure of the telescope. 
   unit of measure type   Units_of_Temperature

   name                   xterm0
   version                1.21
   value data type        ASCII_Real
   description             ShadowCam companding xterm 0 (See appendix in the ShadowCam archive SIS for detailed companding information) 

   name                   xterm1
   version                1.21
   value data type        ASCII_Real
   description             ShadowCam companding xterm 1 (See appendix in the ShadowCam archive SIS for detailed companding information) 

   name                   xterm2
   version                1.21
   value data type        ASCII_Real
   description             ShadowCam companding xterm 2 (See appendix in the ShadowCam archive SIS for detailed companding information) 

   name                   xterm3
   version                1.21
   value data type        ASCII_Real
   description             ShadowCam companding xterm 3 (See appendix in the ShadowCam archive SIS for detailed companding information) 

   name                   xterm4
   version                1.21
   value data type        ASCII_Real
   description             ShadowCam companding xterm 4 (See appendix in the ShadowCam archive SIS for detailed companding information) 

   name                   yaw_flip_angle
   version                1.21
   value data type        ASCII_Integer
   description            The spacecraft is yaw-rotated to ±45° (i.e., 45° or 225°) relative to the reference axis

Parsed Input - Classes:

   name                   SHADOWCAM_Parameters
   description            The SHADOWCAM_Parameters class is the container for ShadowCam-specific observation parameters.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      kplo.rationale_desc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.data_quality_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.data_quality_desc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.dqi_corruption_detected
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.dqi_fpa_out_of_bounds
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.dqi_under_saturated
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.dqi_missing_data
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.dqi_missing_spice
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.dqi_uncalibratable
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.execution_spacecraft_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.execution_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.start_time_offset
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.preroll_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.temperature_fpa_a
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.temperature_fpa_b
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.temperature_fpga
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.temperature_telescope
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.line_rate_ms
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.line_rate_code
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.klines
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.preroll_lines
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.bterm1
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.bterm2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.bterm3
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.bterm4
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.bterm5
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.xterm0
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.xterm1
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.xterm2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.xterm3
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.xterm4
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.mode_test
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.tdi_direction
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.gain_ch0
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.gain_ch1
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.gain_ch2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.gain_ch3
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.gain_ch4
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.gain_ch5
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.offset_ch0
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.offset_ch1
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.offset_ch2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.offset_ch3
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.offset_ch4
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.offset_ch5
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.bias_spread
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.bias_spread_ch0
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.bias_spread_ch1
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.bias_spread_ch2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.bias_spread_ch3
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.bias_spread_ch4
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.bias_spread_ch5
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.data_quality_desc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   LUTI_Parameters
   description            The LUTI_Parameters class is the container for Lunar Terrain Imager A and B specific observation parameters.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      kplo.rationale_desc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.luti_target_type
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      kplo.luti_target_name
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      kplo.frame_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.luti_constant_time_offset
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.spacecraft_clock_start_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.spacecraft_clock_stop_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.line_integration_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.ccd_direction
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.bit_selection
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.pre_scan_mode_selection
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.luti_quality_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.compression_mode
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.compression_ratio
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.constant_offset_data
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.line_rate
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.line_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.temperature_case_start
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.temperature_case_end
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.temperature_ccd_start
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.temperature_ccd_end
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.temperature_fpe_start
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.temperature_fpe_end
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.temperature_psu_start
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.temperature_psu_end
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   KPLO_Parameters
   description            The KPLO_Parameters class is the container for mission-specific metadata elements.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      kplo.product_version_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.mission_phase_name
      minimum occurrences   0
      maximum occurrences   unbounded
      reference type        attribute_of

      local identifier      kplo.orbit_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.producer_institution_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.yaw_flip_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      kplo.SHADOWCAM_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      kplo.LUTI_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

End of Report
