PDS4 Local Data Dictionary Processing Report

Configuration:
   LDDTool Version        16.0.0
   LDD Version Id:        1.0.5.0
   LDD Label Version Id:  1.22
   LDD Discipline (T/F):  false
   LDD Namespace URL:     http://pds.nasa.gov/pds4/
   LDD URN Prefix:        urn:nasa:pds:
   Time                   Wed Dec 03 15:56:16 UTC 2025
   Common Schema          [PDS4_PDS_1G00.xsd]
   Common Schematron      [PDS4_PDS_1G00.sch]
   IM Version Id:         1.16.0.0
   IM Namespace Id:       pds
   IM Label Version Id:   1.22
   IM Object Model        [UpperModel.pont]
   IM Data Dictionary     [dd11179.pins]
   IM Glossary            [Glossary.pins]
   IM Document Spec       [DMDocument.pins]

Parameters:
   Input File             [/home/runner/work/ldd-lro/ldd-lro/src/PDS4_LRO_IngestLDD.xml]
   PDS Processing         true
   LDD Processing         true
   Discipline LDD         false
   Mission LDD            true
   Write Attr Elements    false
   Merge with Master      false

Summary:
   Classes                9
   Attributes             151
   Associations           159
   Error messages         0
   Warning messages       0
   Information messages   0

Detailed validation messages

Parsed Input - Header:
   LDD Name               LRO
   LDD Version            1.0.5.0
   Full Name              Jennifer Ward
   Steward                geo
   Namespace Id           lro
   Comment                
        The LRO dictionary contains classes that describe aspects of the 
        Lunar Reconnaissance Orbiter mission and related instruments.
    
   Last Modification Time 2025-02-01T03:42Z
   PDS4 Merge Flag        false

Parsed Input - Attributes:

   name                   a_axis_radius
   version                1.16
   value data type        ASCII_Real
   description            The a_axis_radius attribute provides the radius of the equatorial axis of the ellipsoid. The IAU calls this "Subplanetary equatorial radius" and mapping applications generally call this "semi_major_axis". 
   minimum value          0.0
   unit of measure type   Units_of_Length

   name                   attenuator
   version                1.16
   value data type        ASCII_Integer
   description            Receiver attenuator setting in decibels.
   minimum value          0
   maximum value          62

   name                   azimuth_beamwidth
   version                1.16
   value data type        ASCII_Real
   description            The null to null main lobe beam pattern beamwidth in azimuth direction.
   unit of measure type   Units_of_Angle

   name                   azimuth_resolution
   version                1.16
   value data type        ASCII_Real
   description            The true resolution of the radar image in the azimuth (along track) direction, evaluated at the center of the image for the transmit, receive, and processing parameters used for the sequence.
   minimum value          0
   maximum value          450
   unit of measure type   Units_of_Length

   name                   b_axis_radius
   version                1.16
   value data type        ASCII_Real
   description            The b_axis_radius attribute provides the value of the intermediate axis of the ellipsoid that defines the approximate shape of a target body. The b_axis_radius is usually in the equatorial plane. The IAU calls this axis "along orbit equatorial radius". Mapping applications, which generally only define a sphere or an ellipse, do not support this radius parameter.
   minimum value          0.0
   unit of measure type   Units_of_Length

   name                   background_offset
   version                1.16
   value data type        ASCII_Integer
   description            The background offset

   name                   band_code
   version                1.16
   value data type        ASCII_Integer
   description            The band_code records the commanded band code for a WAC observation.

   name                   band_description
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The band_description contains a description of a specific band in a MiniRF multibanded 3D image

   name                   band_frequency
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Indicates the frequency band used for the collect. Either 'S' band or 'X' band.

   name                   band_name
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The band_name contains a string identifying the common name for a specific band in a MiniRF multibanded 3D image

   name                   band_sequence_number
   version                1.16
   value data type        ASCII_Integer
   description            The band_sequence_number records the index for a specific band in a MiniRF multibanded 3D image. Index starts at 1

   name                   baq_sample_size
   version                1.16
   value data type        ASCII_Integer
   description            The number of bits used in the BAQ encoding algorithm.
   minimum value          2
   maximum value          12

   name                   begin_temperature_fpa
   version                1.16
   value data type        ASCII_Real
   description            Set to the temperature of the LROC FPA in degrees Celsius, as converted from the raw engineering counts, at the beginning of a series of WAC frames.
   unit of measure type   Units_of_Temperature

   name                   begin_temperature_fpa_raw
   version                1.16
   value data type        ASCII_Integer
   description            Set to the raw engineering counts for the LROC (F)ocal (P)lane (A)rray at the beginning of a series of WAC frames.

   name                   begin_temperature_scs
   version                1.16
   value data type        ASCII_Real
   description            Set to the temperature of the LROC SCS in degrees Celsius, as converted from the raw engineering counts, at the beginning of a series of WAC frames.
   unit of measure type   Units_of_Temperature

   name                   begin_temperature_scs_raw
   version                1.16
   value data type        ASCII_Integer
   description            Set to the raw engineering counts for the LROC SCS at the beginning of a series of WAC frames.

   name                   bterm1
   version                1.16
   value data type        ASCII_Integer
   description            NAC companding bterm 1

   name                   bterm2
   version                1.16
   value data type        ASCII_Integer
   description            NAC companding bterm 2

   name                   bterm3
   version                1.16
   value data type        ASCII_Integer
   description            NAC companding bterm 3

   name                   bterm4
   version                1.16
   value data type        ASCII_Integer
   description            NAC companding bterm 4

   name                   bterm5
   version                1.16
   value data type        ASCII_Integer
   description            NAC companding bterm 5

   name                   bursts
   version                1.16
   value data type        ASCII_Integer
   description            Number of bursts per Mini-RF collect
   minimum value          0
   maximum value          10000

   name                   c_axis_radius
   version                1.16
   value data type        ASCII_Real
   description            The c_axis_radius attribute provides the value of the polar axis of the ellipsoid that defines the approximate shape of a target body. The c_axis_radius is normal to the plane defined by the a_axis_radius and b_axis_radius. The IAU calls this "polar radius". Mapping applications generally call this "semi_minor_axis" 
   minimum value          0.0
   unit of measure type   Units_of_Length

   name                   calibration_software_ver_id
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The version of calibration software used to generate a data product.
   maximum characters     10

   name                   channel
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description             One of nine Diviner channels. 

   name                   channel_a_offset
   version                1.16
   value data type        ASCII_Integer
   description            Records the commanded NAC channel A offset for either the NAC LEFT or NAC RIGHT.

   name                   channel_b_offset
   version                1.16
   value data type        ASCII_Integer
   description            Records the commanded NAC channel B offset for either the NAC LEFT or NAC RIGHT.

   name                   chirp_bandwidth
   version                1.16
   value data type        ASCII_Real
   description            bandwidth of the chirp signal (max frequency - min frequency). chirp_rate is chip_bandwidth/pulse_width.
   unit of measure type   Units_of_Frequency

   name                   chirp_center_frequency
   version                1.16
   value data type        ASCII_Real
   description            Center frequency of the transmitted chirp signal.
   unit of measure type   Units_of_Frequency

   name                   chirp_pulse_width
   version                1.16
   value data type        ASCII_Real
   description            The period of time over which the linear frequency modulated chirp is transmitted.
   unit of measure type   Units_of_Time

   name                   chirp_rate
   version                1.16
   value data type        ASCII_Real
   description            The linear rate used in the transmitted chirp in Hz/sec.

   name                   chirp_start_frequency
   version                1.16
   value data type        ASCII_Real
   description            Starting frequency of the chirp signal.
   unit of measure type   Units_of_Frequency

   name                   chirp_up
   version                1.16
   value data type        ASCII_Boolean
   description            Indicates whether frequency increases or decreases over time in the transmitted chirp. true= frequency increase. false = frequency decrease.

   name                   compand_code
   version                1.16
   value data type        ASCII_Integer
   description            Indicates which stored companding table was used (0-7)
   minimum value          0
   maximum value          7

   name                   complete_lines
   version                1.16
   value data type        ASCII_Integer
   description            The number of lines of data in a data product that are complete; that is, with no missing data.
   minimum value          0

   name                   compression_flag
   version                1.16
   value data type        ASCII_Integer
   description            Indicates if lossless compression was commanded (0=no, 1=yes)
   minimum value          0
   maximum value          1

   name                   coordinate_system_name
   version                1.16
   value data type        ASCII_Text_Preserved
   description            The given name of the used coordinate system. e.g. "MEAN EARTH/POLAR AXIS OF DE421"

   name                   coordinate_system_type
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            There are three basic types of coordinate systems: body-fixed rotating, body-fixed non-rotating, and inertial. A body-fixed coordinate system is one associated with the body (e.g., a planet or satellite). The body-fixed system is centered on the body and rotates with the body (unless it is a non-rotating type), whereas an inertial coordinate system is fixed at some point in space. Currently, the PDS has specifically defined two types of body-fixed rotating coordinate systems: planetocentric and planetographic. However, the set of related data elements are modeled such that definitions for other body-fixed rotating coordinate systems, body-fixed non-rotating and inertial coordinate systems can be added as the need arises. Contact a PDS data engineer for assistance in defining a specific coordinate system. 
   minimum characters     8
   maximum characters     25

   name                   dac_reset_level
   version                1.16
   value data type        ASCII_Integer
   description            Records the commanded DAC reset level for either the NAC LEFT or NAC RIGHT.

   name                   data_quality_desc
   version                1.16
   value data type        ASCII_Text_Collapsed
   description            The data_quality_desc attribute describes the data qualities associated with a data_quality_id attribute. 

   name                   data_quality_id
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The data_quality_id attribute provides a numeric key which identifies the quality of data available for a particular time period. The data_quality_id scheme is unique to a given instrument and is described by the associated data_quality_desc attribute. 

   name                   dlre_date_max
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Gives the maximum recorded date value in a DLRE RDR data product.
   minimum characters     11
   maximum characters     11

   name                   dlre_date_min
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Gives the minimum recorded date value in a DLRE RDR data product.
   minimum characters     11
   maximum characters     11

   name                   dlre_geom_version_id
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The version of Diviner geometry and averaging software used to generate a Diviner GDR product. Example value: 1.0. 
   maximum characters     10

   name                   dlre_instrument_mode_id
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Diviner instrument operating mode.
   maximum characters     20

   name                   dlre_orientation
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            An unordered set of all orientations recorded from activity flags in a DLRE RDR data product. 
   maximum characters     30

   name                   dlre_utc_max
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Gives the maximum recorded UTC value in a DLRE RDR data product.
   minimum characters     12
   maximum characters     12

   name                   dlre_utc_min
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Gives the minimum recorded UTC value in a DLRE RDR data product.
   minimum characters     12
   maximum characters     12

   name                   dlre_wavelength_max
   version                1.16
   value data type        ASCII_Real
   description            Identifies the maximum wavelength at which an observation can be made or was made.
   unit of measure type   Units_of_Length

   name                   dlre_wavelength_min
   version                1.16
   value data type        ASCII_Real
   description            Identifies the minimum wavelength at which an observation can be made or was made.
   unit of measure type   Units_of_Length

   name                   dreb_flight_software_ver_id
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The version of Diviner Remote Electronics Box flight software used to acquire the telemetry data for a data product. 
   maximum characters     10

   name                   end_temperature_fpa
   version                1.16
   value data type        ASCII_Real
   description            Set to the temperature of the LROC FPA in degrees Celsius, as converted from the raw engineering counts, at the end of a series of WAC frames.
   unit of measure type   Units_of_Temperature

   name                   end_temperature_fpa_raw
   version                1.16
   value data type        ASCII_Integer
   description            Set to the raw engineering counts for the LROC (F)ocal (P)lane (A)rray at the end of a series of WAC frames.

   name                   end_temperature_scs
   version                1.16
   value data type        ASCII_Real
   description            Set to the temperature of the LROC SCS in degrees Celsius, as converted from the raw engineering counts, at the end of a series of WAC frames.
   unit of measure type   Units_of_Temperature

   name                   end_temperature_scs_raw
   version                1.16
   value data type        ASCII_Integer
   description            Set to the raw engineering counts for the LROC SCS at the end of a series of WAC frames.

   name                   experiment_id
   version                1.16
   value data type        ASCII_Integer
   description            Identifier used to distinguish between monostatic data collects. Unused in bistatic observations.
   minimum value          0
   maximum value          65536

   name                   exposure_code
   version                1.16
   value data type        ASCII_Integer
   description            Records the commanded exposure code for a WAC observation.

   name                   file_state
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Indicates whether a file possibly contains potentially corrupted data.
   minimum characters     5
   maximum characters     5

   name                   flight_software_version_id
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Identifies the version of the instrument flight software used to acquire the data.
   maximum characters     10

   name                   frame_id
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            For NAC, records if the image was acquired from the "LEFT" or "RIGHT" NAC.

   name                   grid_resolution_height
   version                1.16
   value data type        ASCII_Real
   description            vertical resolution of the grid used to generate the bistatic raw sar data.
   unit of measure type   Units_of_Length

   name                   grid_resolution_width
   version                1.16
   value data type        ASCII_Real
   description            horizontal resolution of the grid used to generate the bistatic raw sar data.
   unit of measure type   Units_of_Length

   name                   image_name
   version                1.16
   value data type        ASCII_Short_String_Preserved
   description            Records the name of the parameter stored in the Diviner image.

   name                   instrument_mode_id
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Records the commanded WAC mode: BW, COLOR, VIS or UV.

   name                   interburst_delay
   version                1.16
   value data type        ASCII_Real
   description            The period of delay between bursts, measured from the start of the last pulse in the previous burst to the start of the first pulse in the next burst.
   unit of measure type   Units_of_Time

   name                   interframe_delay
   version                1.16
   value data type        ASCII_Real
   description            Set to the value of the interframe delay between WAC framelets. Keyword can have values between 25/64 and 280/64 seconds, in 1/64 seconds increments.
   unit of measure type   Units_of_Time

   name                   interframe_gap_code
   version                1.16
   value data type        ASCII_Integer
   description            Records the commanded interframe gap code for a WAC observation.

   name                   latitude_type
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The latitude_type attribute defines the type of latitude (planetographic, planetocentric) used within a cartographic product and as reflected in attribute values within associated PDS labels. For planets and satellites, latitude is measured north and south of the equator; north latitudes are designated as positive. The planetocentric latitude is the angle between the equatorial plane and a line from the center of the body. The planetographic latitude is the angle between the equatorial plane and a line that is normal to the body. In summary, both latitudes are equivalent on a sphere (i.e., equatorial radius equal to polar radius); however, they differ on an ellipsoid (e.g., Mars, Earth). For more on latitude_type, please see the IAU publication available here: http://astrogeology.usgs.gov/groups/IAU-WGCCRE

   name                   line_code
   version                1.16
   value data type        ASCII_Integer
   description            Records the commanded value for the number of NAC lines to acquire, in 1024 increments. (LINES = LINES_CODE * 1024)

   name                   line_exposure_code
   version                1.16
   value data type        ASCII_Integer
   description            Index range from 0 to 4095 each corresponding to one LINE_EXPOSURE_DURATION increment.
   minimum value          0
   maximum value          4095

   name                   line_exposure_duration
   version                1.16
   value data type        ASCII_Real
   description             For NAC products, LINE_EXPOSURE_DURATION can have values between 337.6 and 35,281.6 microseconds, in 128/15 microsecond increments (LINE_EXPOSURE_DURATION = [LINE_EXPOSURE_CODE * 128/15] + 337.6) 
   unit of measure type   Units_of_Time

   name                   lola_dem_vers
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Gives the version of the LOLA digital elevation model that was used to locate Diviner footprints for the generation of a Diviner GDR product. Example value: 1.0. 
   maximum characters     10

   name                   lola_instrument_mode_id
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            LOLA instrument operating mode.
   maximum characters     20

   name                   longitude_direction
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The longitude_direction attribute identifies the direction of longitude (e.g. POSITIVE_EAST or POSITIVE_WEST) for a planet. The IAU definition for direction of positive longitude should be adopted: http://astrogeology.usgs.gov/groups/IAU-WGCCRE. Typically, for planets with prograde (direct) rotations, positive longitude direction is to the west. For planets with retrograde rotations, positive longitude direction is to the east. Generally the Positive West longitude_direction is used for planetographic systems and Positive East is used for planetocentric systems. If the data is defined with Spatial_Domain in a manner not recommended by the IAU, there is a optional Secondary_Spatial_Domain section to define a second set of bounding coordinates.
   minimum characters     13
   maximum characters     13

   name                   look_azimuth_angle
   version                1.16
   value data type        ASCII_Real
   description            The East-West look azimuth discrimination angle. This is the angle between the projection of North into the tangent plane of a sphere at the image center point and the vector from subspacecraft point to the image center projected into the plane. It assumes values from 0 to 360, where 0 means North-looking, 90 East-looking, 180 South-looking, and 270 West-looking. 
   minimum value          0
   maximum value          359
   unit of measure type   Units_of_Angle

   name                   lookup_table_type
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Always set to STORED.

   name                   middle_temperature_fpa
   version                1.16
   value data type        ASCII_Real
   description            Set to the temperature of the LROC FPA in degrees Celsius, as converted from the raw engineering counts, at the middle of a series of WAC frames.
   unit of measure type   Units_of_Temperature

   name                   middle_temperature_fpa_raw
   version                1.16
   value data type        ASCII_Integer
   description            Set to the raw engineering counts for the LROC (F)ocal (P)lane (A)rray at the middle of a series of WAC frames.

   name                   middle_temperature_scs
   version                1.16
   value data type        ASCII_Real
   description            Set to the temperature of the LROC SCS in degrees Celsius, as converted from the raw engineering counts, at the middle of a series of WAC frames.
   unit of measure type   Units_of_Temperature

   name                   middle_temperature_scs_raw
   version                1.16
   value data type        ASCII_Integer
   description            Set to the raw engineering counts for the LROC SCS at the middle of a series of WAC frames.

   name                   mission_phase_name
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description             The mission_phase_name attribute provides the mission-defined name of a time period within the mission. 

   name                   missing_lines
   version                1.16
   value data type        ASCII_Integer
   description            The total number of lines of data missing from an image or observation when it was received on Earth.
   minimum value          0

   name                   mode
   version                1.16
   value data type        ASCII_Integer
   description            Set to the mode value as commanded for both NAC and WAC observations.

   name                   mterm1
   version                1.16
   value data type        ASCII_Real
   description            NAC companding mterm 1

   name                   mterm2
   version                1.16
   value data type        ASCII_Real
   description            NAC companding mterm 2

   name                   mterm3
   version                1.16
   value data type        ASCII_Real
   description            NAC companding mterm 3

   name                   mterm4
   version                1.16
   value data type        ASCII_Real
   description            NAC companding mterm 4

   name                   mterm5
   version                1.16
   value data type        ASCII_Real
   description            NAC companding mterm 5

   name                   nframes
   version                1.16
   value data type        ASCII_Integer
   description            Records the commanded number of frames for a WAC observation.

   name                   observation_type
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Identifies the general type of an observation.
   maximum characters     30

   name                   orbit_number
   version                1.16
   value data type        ASCII_NonNegative_Integer
   description            The orbit_number attribute identifies the number of the orbital revolution around a target body. 

   name                   parameter_max
   version                1.16
   value data type        ASCII_Real
   description            The maximum value for the Diviner parameter specified by lro.parameter_name.
   nillable               true

   name                   parameter_min
   version                1.16
   value data type        ASCII_Real
   description            The minimum value for the Diviner parameter specified by lro.parameter_name.
   nillable               true

   name                   parameter_name
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Diviner parameter name.

   name                   partial_lines
   version                1.16
   value data type        ASCII_Integer
   description            The number of lines of data in a data product that contain partial but incomplete data. 

   name                   preroll_time
   version                1.16
   value data type        ASCII_Date_Time_YMD
   description            The UTC time and date at the start of the image acquisition command, corresponding to the acquisition of 1024 lines at the given exposure prior to the actual image acquisition. 

   name                   producer_full_name
   version                1.16
   value data type        ASCII_Short_String_Preserved
   description            The producer_full_name attribute provides the full_name of the individual mainly responsible for the production of a data set. 

   name                   producer_institution_name
   version                1.16
   value data type        ASCII_Short_String_Preserved
   description            The producer_institution_name attribute identifies a university, research center, NASA center, or other institution associated with the production of a data product. 

   name                   product_type
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The product_type attribute indicates the processing level of an individual data product.

   name                   product_version_id
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The product_version_id attribute identifies the version of an individual data product. 

   name                   pulse_repetition_interval
   version                1.16
   value data type        ASCII_Real
   description            Pulse repetition interval of the signal from the transmitter for Mini-RF bistatic operations.
   unit of measure type   Units_of_Time

   name                   pulses_per_burst
   version                1.16
   value data type        ASCII_Integer
   description            Number of pulses per burst.
   minimum value          1
   maximum value          30000

   name                   radiance_max
   version                1.16
   value data type        ASCII_Real
   description            The maximum recorded value of radiance for the channel given by lro:channel in a DLRE RDR data product.
   nillable               true
   minimum value          -1000.0
   maximum value          100000.0 
   unit of measure type   Units_of_Radiance

   name                   radiance_min
   version                1.16
   value data type        ASCII_Real
   description            The minimum recorded value of radiance for the channel given by lro:channel in a DLRE RDR data product. 
   nillable               true
   minimum value          -1000.0
   maximum value          100000.0 
   unit of measure type   Units_of_Radiance

   name                   range_beamwidth
   version                1.16
   value data type        ASCII_Real
   description            The null to null main lobe beam pattern beamwidth along the range direction.
   unit of measure type   Units_of_Angle

   name                   range_gate_start
   version                1.16
   value data type        ASCII_Real
   description            The delay between the start of a pulse and when the receiver opens. 
   minimum value          0.0
   maximum value          2500.0
   unit of measure type   Units_of_Time

   name                   range_resolution
   version                1.16
   value data type        ASCII_Real
   description            The true resolution of the radar image in the range (across track) direction, evaluated at the center of the image for the transmit, receive, and processing parameters used for the sequence. 
   maximum value          450
   unit of measure type   Units_of_Length

   name                   rationale_desc
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The rationale_desc attribute describes the rationale for performing a particular observation.

   name                   receiver_frequency
   version                1.16
   value data type        ASCII_Real
   description            The center of the receiver frequency band, transferred to base band/DC (0Hz) in the instrument data. This combined with a the sampling frequency gives a complete picture of the receiver's frequency configuration. 
   unit of measure type   Units_of_Frequency

   name                   receiver_pulse_width
   version                1.16
   value data type        ASCII_Real
   description            The period of time over which the receiver is open and recording samples
   minimum value          5
   maximum value          2500
   unit of measure type   Units_of_Time

   name                   samples_per_pulse
   version                1.16
   value data type        ASCII_Integer
   description            Number of samples received within a pulse. When operating in the bistatic, receive only mode, the instrument is not pulsing in the traditional sense, but the number of values reported here define a block sent into the BAQ encoding process. Corresponds to the number of rows in the Bistatic raw data table.
   minimum value          0
   maximum value          8192

   name                   sampling_frequency
   version                1.16
   value data type        ASCII_Real
   description            Sampling frequency used to capture samples in the receiver
   nillable               true
   unit of measure type   Units_of_Frequency

   name                   sar_channel
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The channel associated with the data product

   name                   sar_emission_angle
   version                1.16
   value data type        ASCII_Real
   description            The angle between the normal to the lunar surface (body radius based on a digital elevation model or DEM) and the vector to the receiver.
   unit of measure type   Units_of_Angle

   name                   sar_incidence_angle
   version                1.16
   value data type        ASCII_Real
   description            The angle between the normal to the lunar surface (body radius based on a digital elevation model or DEM) and the vector to the Earth-based transmitter.
   unit of measure type   Units_of_Angle

   name                   sar_instrument_mode_id
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Mini-RF SAR instrument operating mode.
   maximum characters     20

   name                   sar_phase_angle
   version                1.16
   value data type        ASCII_Real
   description            The angle between the SAR (Mini-RF) receiver and the Earth-based transmitter. It is also known as the bistatic angle.
   unit of measure type   Units_of_Angle

   name                   sclk0
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The SCLK latched at Mini-RF bootup. Used as the zero reference for the Mini-RF fine-time fields.

   name                   software_version_id
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The software_version_id element indicates the version (development level) of a program or a program library.
   maximum characters     20

   name                   spacecraft_clock_count_partition
   version                1.16
   value data type        ASCII_NonNegative_Integer
   description            The spacecraft_clock_count_partition attribute indicates the clock partition active for the spacecraft_clock_start_count and spacecraft_clock_stop_count attributes. 

   name                   spacecraft_clock_preroll_count
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Set to the sclk string for the start of an observation preroll acquisition.

   name                   spacecraft_clock_start_count
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_start_count attribute provides the value of the spacecraft clock at the beginning of a time period of interest. 

   name                   spacecraft_clock_stop_count
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_stop_count attribute provides the value of the spacecraft clock at the beginning of a time period of interest. 

   name                   start_orbit_number
   version                1.16
   value data type        ASCII_Real
   description            Provides the the lowest revolution orbit number that contributed data to a given data product. 

   name                   start_solar_longitude
   version                1.16
   value data type        ASCII_Real
   description            Marks the beginning of a time range measured in solar longitude. Solar longitude is the value of the angle between the body_Sun line at the time of interest and the body_Sun line at the vernal equinox, thus providing a measure of the season on the target body. 
   minimum value          -180
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   stcf_file_name
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Provides the name of the LRO Spacecraft Time Correlation file, which is a housekeeping file containing the offset between the spacecraft raw clock and terrestrial time. The time correlation file is used to compute the start and stop spacecraft clock times for LOLA data products. 
   maximum characters     40

   name                   stop_orbit_number
   version                1.16
   value data type        ASCII_Real
   description            Provides the the highest revolution orbit number that contributed data to a given data product. 

   name                   stop_solar_longitude
   version                1.16
   value data type        ASCII_Real
   description            Marks the end of a time range measured in solar longitude. Solar longitude is the value of the angle between the body_Sun line at the time of interest and the body_Sun line at the vernal equinox, thus providing a measure of the season on the target body. 
   minimum value          -180
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   sub_spacecraft_ground_azimuth
   version                1.16
   value data type        ASCII_Real
   description            Provides the value of the angle, measured on the target body surface, between the direction from a ground point to the north pole and the direction from the ground point to the sub-spacecraft point. If the location of the ground point at which the azimuth is measured is not otherwise specified, it is assumed to correspond to the center of the image. The values of this angle increase in a clockwise direction. When a pair of values is given, e.g. (350.0, 10.0), they represent the ordered end-members of a range of ground azimuth values that extends clockwise from the first to the second, modulo 360 degrees. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   tb_max
   version                1.16
   value data type        ASCII_Real
   description            The maximum recorded value of brightness temperature for the channel given by lro:channel in a DLRE RDR data product. 
   nillable               true
   minimum value          -450.0
   maximum value          10000.0
   unit of measure type   Units_of_Temperature

   name                   tb_min
   version                1.16
   value data type        ASCII_Real
   description            The minimum recorded value of brightness temperature for the channel given by lro:channel in a DLRE RDR data product. 
   nillable               true
   minimum value          -450.0
   maximum value          10000.0
   unit of measure type   Units_of_Temperature

   name                   temperature_fpa
   version                1.16
   value data type        ASCII_Real
   description            Set to the temperature of the LROC FPA in degrees Celsius, as converted from the raw engineering counts.
   unit of measure type   Units_of_Temperature

   name                   temperature_fpa_raw
   version                1.16
   value data type        ASCII_Integer
   description            Set to the raw engineering counts for the LROC (F)ocal (P)lane (A)rray.

   name                   temperature_fpga
   version                1.16
   value data type        ASCII_Real
   description            Set to the temperature of the LROC FPGA in degrees Celsius, as converted from the raw engineering counts.
   unit of measure type   Units_of_Temperature

   name                   temperature_fpga_raw
   version                1.16
   value data type        ASCII_Integer
   description            Set to the raw engineering counts for the LROC (F)ield (P)rogrammable (G)ate (A)rray.

   name                   temperature_scs
   version                1.16
   value data type        ASCII_Real
   description            Set to the temperature of the LROC SCS in degrees Celsius, as converted from the raw engineering counts.
   unit of measure type   Units_of_Temperature

   name                   temperature_scs_raw
   version                1.16
   value data type        ASCII_Integer
   description            Set to the raw engineering counts for the LROC SCS.

   name                   temperature_telescope
   version                1.16
   value data type        ASCII_Real
   description            Set to the temperature of the LROC telescope corresponding to NAC-L or NAC-R, as converted from the raw engineering counts.
   unit of measure type   Units_of_Temperature

   name                   temperature_telescope_raw
   version                1.16
   value data type        ASCII_Integer
   description            Set to the raw engineering counts for the LROC Telescope corresponding to NAC-L or NAC-R.

   name                   total_lines
   version                1.16
   value data type        ASCII_Integer
   description            The total number of lines of data in a data product, including both complete lines and partial lines.

   name                   total_pulse_count
   version                1.16
   value data type        ASCII_Integer
   description            The total number of pulses contained in the Mini-RF raw data product.

   name                   transmit_polarization
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Specifies the polarization of the transmitted signal.

   name                   transmitter
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            Specifies the transmitting radar platform, including the Mini-RF transmitter when it was operational.

   name                   transmitter_eirp
   version                1.16
   value data type        ASCII_Real
   description            Effective isotropic radiated power from transmitter; units are decibels-milliwatt-isotropic.

   name                   transmitter_range
   version                1.16
   value data type        ASCII_Real
   description            Mean range from the transmitter location to the lunar surface at the Mini-RF boresight intercept
   unit of measure type   Units_of_Length

   name                   upload_id
   version                1.16
   value data type        ASCII_Short_String_Collapsed
   description            The upload_id attribute describes a spacecraft command set that is associated with the given data product.

   name                   xterm1
   version                1.16
   value data type        ASCII_Integer
   description            NAC companding xterm 1

   name                   xterm2
   version                1.16
   value data type        ASCII_Integer
   description            NAC companding xterm 2

   name                   xterm3
   version                1.16
   value data type        ASCII_Integer
   description            NAC companding xterm 3

   name                   xterm4
   version                1.16
   value data type        ASCII_Integer
   description            NAC companding xterm 4

   name                   xterm5
   version                1.16
   value data type        ASCII_Integer
   description            NAC companding xterm 5

Parsed Input - Classes:

   name                   LROC_Parameters
   description            The LROC_Parameters class is the container for LROC-specific observation parameters.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lro.upload_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.rationale_desc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.data_quality_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.data_quality_desc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.begin_temperature_scs
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.middle_temperature_scs
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.end_temperature_scs
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.begin_temperature_fpa
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.middle_temperature_fpa
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.end_temperature_fpa
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.begin_temperature_scs_raw
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.middle_temperature_scs_raw
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.end_temperature_scs_raw
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.begin_temperature_fpa_raw
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.middle_temperature_fpa_raw
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.end_temperature_fpa_raw
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.preroll_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.spacecraft_clock_preroll_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.frame_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.temperature_scs
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.temperature_fpa
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.temperature_fpga
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.temperature_telescope
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.temperature_scs_raw
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.temperature_fpa_raw
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.temperature_fpga_raw
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.temperature_telescope_raw
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.exposure_code
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.interframe_delay
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.instrument_mode_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.lookup_table_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.line_exposure_duration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.line_exposure_code
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.dac_reset_level
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.channel_a_offset
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.channel_b_offset
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.compand_code
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.line_code
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.bterm1
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.bterm2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.bterm3
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.bterm4
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.bterm5
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.mterm1
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.mterm2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.mterm3
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.mterm4
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.mterm5
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.xterm1
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.xterm2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.xterm3
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.xterm4
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.xterm5
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.compression_flag
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.mode
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.nframes
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.band_code
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.interframe_gap_code
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.background_offset
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Parameter_Range
   description            The Parameter_Range class contains the minimum and maximum values of Diviner parameters.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lro.parameter_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.parameter_min
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.parameter_max
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Channel_Range
   description            The Channel_Range class contains spectral parameters for specific Diviner channels.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lro.channel
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.radiance_min
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.radiance_max
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.tb_min
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.tb_max
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   MiniRF_Band
   description            The MiniRF_Band class contains the name and description for a specific band in a MiniRF Array_3D_Image
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lro.band_name
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.band_description
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.band_sequence_number
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

   name                   Diviner_Parameters
   description            The Diviner_Parameters class is the container for Diviner-specific observation parameters.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lro.missing_lines
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.partial_lines
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.complete_lines
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.total_lines
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.file_state
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.flight_software_version_id
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      lro.dreb_flight_software_ver_id
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      lro.lola_dem_vers
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.dlre_geom_version_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.calibration_software_ver_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.software_version_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.dlre_date_min
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.dlre_date_max
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.dlre_utc_min
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.dlre_utc_max
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.dlre_wavelength_min
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.dlre_wavelength_max
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.dlre_orientation
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      lro.observation_type
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      lro.dlre_instrument_mode_id
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      lro.image_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.Parameter_Range
      minimum occurrences   0
      maximum occurrences   *
      reference type        component_of

      local identifier      lro.Channel_Range
      minimum occurrences   0
      maximum occurrences   *
      reference type        component_of

   name                   MiniRF_Parameters
   description            The MiniRF_Parameters class is the container for MiniRF-specific observation parameters.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lro.experiment_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.pulse_repetition_interval
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.chirp_pulse_width
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.chirp_rate
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.chirp_start_frequency
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.chirp_up
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.chirp_bandwidth
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.chirp_center_frequency
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.receiver_frequency
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.samples_per_pulse
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.range_gate_start
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.receiver_pulse_width
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.interburst_delay
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.bursts
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.pulses_per_burst
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.total_pulse_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.attenuator
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.band_frequency
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.sar_channel
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.sampling_frequency
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.baq_sample_size
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.sclk0
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.transmitter
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.sar_instrument_mode_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.transmitter_eirp
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.transmitter_range
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.look_azimuth_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.sar_incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.sar_emission_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.sar_phase_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.azimuth_beamwidth
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.range_beamwidth
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.sub_spacecraft_ground_azimuth
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.azimuth_resolution
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.range_resolution
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.grid_resolution_height
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.grid_resolution_width
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.transmit_polarization
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.MiniRF_Band
      minimum occurrences   0
      maximum occurrences   *
      reference type        component_of

   name                   LOLA_Parameters
   description            The LOLA_Parameters class is the container for LOLA-specific observation parameters.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lro.lola_instrument_mode_id
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      lro.stcf_file_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Geodetic_Model
   description            The Geodetic_Model class provides parameters describing the shape of the planet.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lro.latitude_type
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.a_axis_radius
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.b_axis_radius
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.c_axis_radius
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.longitude_direction
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.coordinate_system_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.coordinate_system_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   LRO_Parameters
   description            The LRO_Parameters class is the container for mission-specific metadata elements.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lro.product_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.product_version_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.orbit_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.start_orbit_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.stop_orbit_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.start_solar_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.stop_solar_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.mission_phase_name
      minimum occurrences   0
      maximum occurrences   unbounded
      reference type        attribute_of

      local identifier      lro.spacecraft_clock_count_partition
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.spacecraft_clock_start_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.spacecraft_clock_stop_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.producer_full_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.producer_institution_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lro.LROC_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      lro.Diviner_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      lro.MiniRF_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      lro.LOLA_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      lro.Geodetic_Model
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

End of Report
