PDS4 Local Data Dictionary Processing Report

Configuration:
   LDDTool Version        16.1.3
   LDD Version Id:        1.0.1.0
   LDD Label Version Id:  1.24
   LDD Discipline (T/F):  false
   LDD Namespace URL:     http://pds.nasa.gov/pds4/
   LDD URN Prefix:        urn:nasa:pds:
   Time                   Tue Jun 16 18:00:24 UTC 2026
   Common Schema          [PDS4_PDS_1I00.xsd]
   Common Schematron      [PDS4_PDS_1I00.sch]
   IM Version Id:         1.18.0.0
   IM Namespace Id:       pds
   IM Label Version Id:   1.24
   IM Object Model        [UpperModel.pont]
   IM Data Dictionary     [dd11179.pins]
   IM Glossary            [Glossary.pins]
   IM Document Spec       [DMDocument.pins]

Parameters:
   Input File             [/home/runner/work/ldd-lucy/ldd-lucy/src/PDS4_LUCY_IngestLDD.xml]
   PDS Processing         true
   LDD Processing         true
   Discipline LDD         false
   Mission LDD            true
   Write Attr Elements    false
   Merge with Master      false

Summary:
   Classes                11
   Attributes             94
   Associations           103
   Error messages         0
   Warning messages       0
   Information messages   0

Detailed validation messages

Parsed Input - Header:
   LDD Name               Lucy Mission LDD
   LDD Version            1.0.1.0
   Full Name              Crombie, M. Katherine
   Steward                katecrombie
   Namespace Id           lucy
   Comment                _TBD_Ingest_LDD
   Last Modification Time 2025-07-17
   PDS4 Merge Flag        false

Parsed Input - Attributes:

   name                   observation_id
   version                1.18
   value data type        ASCII_Integer
   description            The Lucy Mission observation identifier. 
   minimum value          0
   maximum value          99999

   name                   observation_id_count
   version                1.18
   value data type        ASCII_Integer
   description            The Lucy Mission observation identifier counter. This number increments by 1 with each planned observation sequence (L'LORRI only). 
   minimum value          0
   maximum value          99999

   name                   observation_complete
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The Lucy Mission observation completion status. 

   name                   observation_missing_packets
   version                1.18
   value data type        ASCII_NonNegative_Integer
   description            The number of missing packets in the observation. The best data quality has no missing packets. 

   name                   start_sclk
   version                1.18
   value data type        ASCII_Real
   description            The Lucy spacecraft clock (SCLK) time (in seconds) at the start of the observation. 
   unit of measure type   Units_of_Time

   name                   mid_sclk
   version                1.18
   value data type        ASCII_Real
   description            The Lucy spacecraft clock (SCLK) time (in seconds) at the mid-time of the observation. 
   unit of measure type   Units_of_Time

   name                   stop_sclk
   version                1.18
   value data type        ASCII_Real
   description            The Lucy spacecraft clock (SCLK) time (in seconds) at the end of the observation. 
   unit of measure type   Units_of_Time

   name                   mid_utc
   version                1.18
   value data type        ASCII_Date_Time_YMD_UTC
   description            The middle time of the observation in ISO UTC format "YYYY-MM-DDTHH:MM:SS.sss" 

   name                   mid_sclk_string
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The middle time of the observation in Lucy spacecraft clock string partition/SSSSSSSSSS-PPPPP, where S is seconds and P are ticks in units of 1/66535 of a second. 

   name                   mid_utc_doy
   version                1.18
   value data type        ASCII_Date_Time_DOY_UTC
   description            The middle time of the observation in ISO DOY format, YYYY-DOYTHH:MM:SS.sss

   name                   mid_utc_jd
   version                1.18
   value data type        ASCII_Real
   description            The middle time of the observation in Julian day format.
   unit of measure type   Units_of_Time

   name                   mid_ephemeris_time
   version                1.18
   value data type        ASCII_Real
   description            The middle time of the observation in ephemeris time, seconds past J2000, TDB.
   unit of measure type   Units_of_Time

   name                   ccsds_sclk_time
   version                1.18
   value data type        ASCII_Integer
   description            The Lucy spacecraft clock time of the CCSDS playback timestamp in seconds.
   unit of measure type   Units_of_Time

   name                   load_identifier
   version                1.18
   value data type        ASCII_Integer
   description            The command sequence load identifier
   nillable               true
   minimum value          21289
   maximum value          99999

   name                   mission_segment
   version                1.18
   value data type        ASCII_Short_String_Preserved
   description            The Lucy Mission segment

   name                   sap_identifier
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The Lucy Mission science activity plan identifier.
   nillable               true

   name                   visit_name
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The Lucy Mission trojan asteroid visit name.
   nillable               true

   name                   instrument_side
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The Lucy elctronics side.

   name                   llorri_status
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The status of the L'LORRI instrument.

   name                   lralph_status
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The status of the L'RALPH instrument.

   name                   ltes_status
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The status of the L'TES instrument.

   name                   ttcam_status
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The status of the TTCAM instrument.

   name                   target_fov_count
   version                1.18
   value data type        ASCII_Integer
   description            The number of possible targets in FOV (SPICE-derived).

   name                   target_fov_name
   version                1.18
   value data type        ASCII_Short_String_Preserved
   description            The name of the possible target in FOV (SPICE-derived).

   name                   internal_product_version_id
   version                1.18
   value data type        ASCII_Integer
   description            The Lucy pipeline internal data processing version number. This number is likely to be grater than the PDS version number given in the version_id attribute in the Observation_Area.

   name                   attached_sync_marker_dec
   version                1.18
   value data type        ASCII_Integer
   description            Attached Sync Marker, decimal representation.

   name                   attached_sync_marker_hex
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            Attached Sync Marker, hexidecimal representation.

   name                   latch_count
   version                1.18
   value data type        ASCII_Integer
   description            The number of times a latchup has occurred.
   minimum value          0

   name                   calibration_lamp_level_1
   version                1.18
   value data type        ASCII_Integer
   description            The Digital Number (DN) setting for calibration lamp one.
   unit of measure type   Units_of_Misc

   name                   calibration_lamp_level_2
   version                1.18
   value data type        ASCII_Integer
   description            The Digital Number (DN) setting for calibration lamp two.
   unit of measure type   Units_of_Misc

   name                   bias_level
   version                1.18
   value data type        ASCII_Real
   description            The lucy:bias_level attribute appears in calibrated L'LORRI data products and contains the mean bias level of the detector's dark columns.
   minimum value          0
   unit of measure type   Units_of_Misc

   name                   read_noise
   version                1.18
   value data type        ASCII_Real
   description            The lucy:read_noise attribute appears in calibrated L'LORRI data products and provides the CCD read noise for the image.
   minimum value          0
   unit of measure type   Units_of_Misc

   name                   ccd_gain
   version                1.18
   value data type        ASCII_Real
   description            The lucy:ccd_gain attribute appears in calibrated L'LORRI data products and provides the CCD gain setting for the image.
   minimum value          0
   unit of measure type   Units_of_Misc

   name                   bias_offset
   version                1.18
   value data type        ASCII_Real
   description            The lucy:bias_offset attribute appears in calibrated L'LORRI data products and provides the CCD bias offset between the active and inactive regions of the detector.
   minimum value          0
   unit of measure type   Units_of_Misc

   name                   frame_transfer_scrub_time
   version                1.18
   value data type        ASCII_Real
   description             The lucy:frame_transfer_scrub_time attribute appears in calibrated L'LORRI data products and contains the instrument's frame transfer/scrub time. For the L'LORRI instrument, these two quantities (transfer and scrub times) are exactly equal. 
   minimum value          11.0
   maximum value          12.0
   unit of measure type   Units_of_Time

   name                   playback_start
   version                1.18
   value data type        ASCII_Integer
   description            Playback science header timstamp of the first m4 packet used in spacecraft clock seconds.
   unit of measure type   Units_of_Time

   name                   playback_end
   version                1.18
   value data type        ASCII_Integer
   description            Playback science header timstamp of the last m4 packet used in spacecraft clock seconds.
   unit of measure type   Units_of_Time

   name                   playback_bad_pixel_mask_status
   version                1.18
   value data type        ASCII_Boolean
   description            Status of the bad pixel map, true or false

   name                   playback_truncation_status
   version                1.18
   value data type        ASCII_Boolean
   description            Status of the truncation enabled, true or false

   name                   playback_header_type
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            Defines what type of science data is being played from the Ralph instrument memory to the spacecraft.

   name                   test_pattern_setting
   version                1.18
   value data type        ASCII_Integer
   description            The instrument test pattern setting, 0 is science, 1 is test pattern.
   minimum value          0
   maximum value          2

   name                   hs_xtrack_start_row
   version                1.18
   value data type        ASCII_Integer
   description            The cross track start row from the high speed header.

   name                   scan_row_pixels
   version                1.18
   value data type        ASCII_Integer
   description            The number of pixels in the scan row.
   minimum value          1

   name                   fpecrc_error_flag
   version                1.18
   value data type        ASCII_Boolean
   description            FPE checksum error flag, true or false

   name                   m4_calibration_state
   version                1.18
   value data type        ASCII_Integer
   description            Calibration state (TBR)

   name                   m4_blackbody_setting
   version                1.18
   value data type        ASCII_Integer
   description            Blackbody state (TBR)

   name                   m4_filament_setting
   version                1.18
   value data type        ASCII_Integer
   description            Filament setting (TBR)

   name                   fpe_drop_frames
   version                1.18
   value data type        ASCII_NonNegative_Integer
   description            Number of FPE drop frames (TBR).

   name                   mce_scan_rate
   version                1.18
   value data type        ASCII_Real
   description            The MCE scan rate (TBR).
   unit of measure type   Units_of_Angular_Velocity

   name                   first_packet_timestamp
   version                1.18
   value data type        ASCII_Real
   description            The timestamp of the first packet recorded in spacraft clock seconds.
   unit of measure type   Units_of_Time

   name                   last_packet_timestamp
   version                1.18
   value data type        ASCII_Real
   description            The timestamp of the last packet recorded in spacraft clock seconds.
   unit of measure type   Units_of_Time

   name                   xsum_error_flag_status
   version                1.18
   value data type        ASCII_Boolean
   description            Xsum flag indicating if there are errors in the stored data packet, true or false

   name                   lr_acquisition_start_block
   version                1.18
   value data type        ASCII_Integer
   description            The L'Ralph observation acquisition start block address.
   nillable               true

   name                   mce_start_position
   version                1.18
   value data type        ASCII_Integer
   description            The MCE start position (TBR), units TBD

   name                   mce_end_position
   version                1.18
   value data type        ASCII_Integer
   description            The MCE start position (TBR), units TBD

   name                   board_selection
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The instrument side selected

   name                   blocks_allocated
   version                1.18
   value data type        ASCII_Integer
   description            The number of blocks allocated
   nillable               true

   name                   mvic_ccd_list
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            List of the MVIC CCDs used in this observation.

   name                   mvic_actual_atrack_summing
   version                1.18
   value data type        ASCII_Integer
   description            MVIC actual along track pixel summing.

   name                   mvic_actual_xtrack_summing
   version                1.18
   value data type        ASCII_Integer
   description            MVIC actual along track pixel summing.

   name                   mvic_planned_atrack_summing
   version                1.18
   value data type        ASCII_Integer
   description            MVIC actual summing mode.

   name                   mvic_planned_xtrack_summing
   version                1.18
   value data type        ASCII_Integer
   description            MVIC planned along track pixel summing.

   name                   mvic_summing_mode
   version                1.18
   value data type        ASCII_Integer
   description            MVIC planned summing mode.

   name                   actual_ccd1_tdi_configuration
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            Actual CCD 1 TDI configuration.

   name                   actual_ccd2_tdi_configuration
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            Actual CCD 2 TDI configuration.

   name                   actual_ccd3_tdi_configuration
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            Actual CCD 3 TDI configuration.

   name                   actual_ccd4_tdi_configuration
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            Actual CCD 4 TDI configuration.

   name                   actual_ccd5_tdi_configuration
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            Actual CCD 5 TDI configuration.

   name                   actual_ccd6_tdi_configuration
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            Actual CCD 6 TDI configuration.

   name                   planned_ccd1_tdi_configuration
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The planned CCD 1 TDI configuration.

   name                   planned_ccd2_tdi_configuration
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The planned CCD 2 TDI configuration.

   name                   planned_ccd3_tdi_configuration
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The planned CCD 3 TDI configuration.

   name                   planned_ccd4_tdi_configuration
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The planned CCD 4 TDI configuration.

   name                   planned_ccd5_tdi_configuration
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The planned CCD 5 TDI configuration.

   name                   planned_ccd6_tdi_configuration
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The planned CCD 6 TDI configuration.

   name                   mvic_fpe_vis_temperature
   version                1.18
   value data type        ASCII_Real
   description            The MVIC FPE VIS Temperature
   unit of measure type   Units_of_Temperature

   name                   mvic_observation_allocation
   version                1.18
   value data type        ASCII_Real
   description            MVIC allocated observation duration
   unit of measure type   Units_of_Time

   name                   mvic_tdi_row_integration_time
   version                1.18
   value data type        ASCII_Real
   description            MVIC allocated observation duration
   unit of measure type   Units_of_Time

   name                   leisa_mode
   version                1.18
   value data type        ASCII_Boolean
   description            LEISA observation mode, T is CDS, F is NONCDS. (TBR)

   name                   leisa_observation_allocation
   version                1.18
   value data type        ASCII_Integer
   description            LEISA observation allocation duration.
   unit of measure type   Units_of_Time

   name                   leisa_integration_time
   version                1.18
   value data type        ASCII_Real
   description            LEISA observation integration time (TBR)
   unit of measure type   Units_of_Time

   name                   leisa_atrack_start_channel
   version                1.18
   value data type        ASCII_Integer
   description            LEISA along track start channel

   name                   leisa_atrack_num_channels
   version                1.18
   value data type        ASCII_Integer
   description            LEISA along track number of channels.

   name                   leisa_xtrack_start_row
   version                1.18
   value data type        ASCII_Integer
   description            LEISA cross track start row.

   name                   leisa_xtrack_num_rows
   version                1.18
   value data type        ASCII_Integer
   description            LEISA cross track number of rows.

   name                   leisa_offset
   version                1.18
   value data type        ASCII_Integer
   description            LEISA offset (TBR)

   name                   leisa_fpa_temperature
   version                1.18
   value data type        ASCII_Real
   description            LEISA Focal Plane Array Temperature
   unit of measure type   Units_of_Temperature

   name                   pivot_wavelength
   version                1.18
   value data type        ASCII_Real
   description             The value contained in the lucy:pivot_wavelength attribute is used when converting L'LORRI calibrated pixel values to physical units. 
   minimum value          0.0
   unit of measure type   Units_of_Length

   name                   solar_constant
   version                1.18
   value data type        ASCII_Real
   description             The lucy:solar_constant attribute supplies the constant to be used for sources with a spectral distribution similar to the Sun to convert calibrated pixel values to physical units. 

   name                   red_trojan_constant
   version                1.18
   value data type        ASCII_Real
   description             The lucy:red_trojan_constant attribute supplies the constant to be used for sources with a spectral distribution similar to that of "red" Trojans to convert calibrated pixel values to physical units. 

   name                   gray_trojan_constant
   version                1.18
   value data type        ASCII_Real
   description             The lucy:gray_trojan_constant attribute supplies the constant to be used for sources with a spectral distribution similar to that of "gray" Trojans to convert calibrated pixel values to physical units. 

   name                   dinkinesh_constant
   version                1.18
   value data type        ASCII_Real
   description             The lucy:dinkinesh_constant attribute supplies the constant to be used for sources with a spectral distribution similar to that of Dinkinesh to convert calibrated pixel values to physical units. 

   name                   photometric_zero_point
   version                1.18
   value data type        ASCII_Real
   description             The lucy:photometric_zero_point attribute supplies the photometric zero point to be used to convert between units of (ir)radiance and visual magnitude, V. 

   name                   units_of_conversion_constants
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description             For resolved sources, the radiometric conversion produces data in units of radiance. For unresolved sources, the conversion results in units of flux (irradiance). The lucy:units_of_conversion_constants attribute contains the appropriate physical units for the conversion constants in the class in which it is contained to produce either radiance or flux units, as appropriate, when the conversion is applied. 

Parsed Input - Classes:

   name                   Diffuse_Source
   description             The lucy:Point_Source class presents radiometric conversion constants for converting calibrated pixel values into physical units for resolved/extended sources. 
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lucy:units_of_conversion_constants
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy:solar_constant
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy:red_trojan_constant
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy:gray_trojan_constant
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy:dinkinesh_constant
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Lucy_Observation_Time_Information
   description            Lucy Mission observation identification and timing information.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lucy.Lucy_Observation_Time_Information.observation_id
      minimum occurrences   1
      maximum occurrences   *
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Time_Information.observation_id_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Time_Information.observation_complete
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Time_Information.observation_missing_packets
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Time_Information.start_sclk
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Time_Information.mid_sclk
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Time_Information.stop_sclk
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Time_Information.mid_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Time_Information.mid_sclk_string
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Time_Information.mid_utc_doy
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Time_Information.mid_utc_jd
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Time_Information.mid_ephemeris_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Time_Information.ccsds_sclk_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Lucy_Observation_Planning
   description            The Lucy Mission observation planning class and attributes describe the observation planning information needed to understand the planned spacecraft observations.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lucy.Lucy_Observation_Planning.load_identifier
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Planning.mission_segment
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Planning.sap_identifier
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Planning.visit_name
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Planning.instrument_side
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Planning.llorri_status
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Planning.lralph_status
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Planning.ltes_status
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Observation_Planning.ttcam_status
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Lucy_Target_List
   description            The Lucy Mission class that contains the target list of potential targets in a given observation.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lucy.Lucy_Target_List.target_fov_count
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.Lucy_Target_List.target_fov_name
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

   name                   Lucy_Product_Information
   description            The Lucy Mission class that contains attributes specific to the labeled data product.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lucy.Lucy_Product_Information.internal_product_version_id
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

   name                   LLORRI_Instrument_Parameters
   description            The Lucy LORRI instrument class that contains instrument specific attributes relevant to the labeled data product.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lucy.LLORRI_Instrument_Parameters.attached_sync_marker_dec
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LLORRI_Instrument_Parameters.attached_sync_marker_hex
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LLORRI_Instrument_Parameters.latch_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LLORRI_Instrument_Parameters.calibration_lamp_level_1
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LLORRI_Instrument_Parameters.calibration_lamp_level_2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LLORRI_Instrument_Parameters.bias_level
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LLORRI_Instrument_Parameters.read_noise
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LLORRI_Instrument_Parameters.ccd_gain
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LLORRI_Instrument_Parameters.bias_offset
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LLORRI_Instrument_Parameters.frame_transfer_scrub_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy:Radiometric_Conversion_Constants
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

   name                   LRalph_Instrument_Common_Parameters
   description            The Lucy LRalph instrument class that contains the common (LEISA and MVIC) instrument specific attributes relevant to the labeled data product.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lucy.LRalph_Instrument_Common_Parameters.playback_start
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.playback_end
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.playback_bad_pixel_mask_status
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.playback_truncation_status
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.playback_header_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.test_pattern_setting
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.hs_xtrack_start_row
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.scan_row_pixels
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.scan_row_pixels
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.fpecrc_error_flag
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.m4_calibration_state
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.m4_blackbody_setting
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.m4_filament_setting
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.fpe_drop_frames
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.mce_scan_rate
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.first_packet_timestamp
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.last_packet_timestamp
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.xsum_error_flag_status
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.lr_acquisition_start_block
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.mce_start_position
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.mce_end_position
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.board_selection
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LRalph_Instrument_Common_Parameters.blocks_allocated
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   LEISA_Instrument_Parameters
   description            The Lucy LRalph LEISA class that contains the instrument specific attributes relevant to the labeled data product.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lucy.LEISA_Instrument_Parameters.leisa_mode
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LEISA_Instrument_Parameters.leisa_observation_allocation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LEISA_Instrument_Parameters.leisa_integration_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LEISA_Instrument_Parameters.leisa_atrack_start_channel
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LEISA_Instrument_Parameters.leisa_atrack_num_channels
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LEISA_Instrument_Parameters.leisa_xtrack_start_row
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LEISA_Instrument_Parameters.leisa_xtrack_num_rows
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LEISA_Instrument_Parameters.leisa_offset
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.LEISA_Instrument_Parameters.leisa_fpa_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   MVIC_Instrument_Parameters
   description            The Lucy LRalph MVIC class that contains the instrument specific attributes relevant to the labeled data product.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lucy.MVIC_Instrument_Parameters.mvic_ccd_list
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.mvic_actual_atrack_summing
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.mvic_actual_xtrack_summing
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.mvic_planned_atrack_summing
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.mvic_planned_xtrack_summing
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.mvic_summing_mode
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.actual_ccd1_tdi_configuration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.actual_ccd2_tdi_configuration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.actual_ccd3_tdi_configuration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.actual_ccd4_tdi_configuration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.actual_ccd5_tdi_configuration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.actual_ccd6_tdi_configuration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.planned_ccd1_tdi_configuration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.planned_ccd2_tdi_configuration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.planned_ccd3_tdi_configuration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.planned_ccd4_tdi_configuration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.planned_ccd5_tdi_configuration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.planned_ccd6_tdi_configuration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.mvic_fpe_vis_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.mvic_observation_allocation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy.MVIC_Instrument_Parameters.mvic_tdi_row_integration_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Point_Source
   description             The lucy:Point_Source class presents radiometric conversion constants for converting calibrated pixel values into physical units for unresolved/point sources. 
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lucy:units_of_conversion_constants
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy:solar_constant
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy:red_trojan_constant
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy:gray_trojan_constant
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy:dinkinesh_constant
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Radiometric_Conversion_Constants
   description             The lucy:Radiometric_Conversion_Constants class provides the values needed to perform the conversion from the calibrated pixel values to physical units. This conversion is dependent on the spectral distribition of the source, the detector wavelength range, and whether or not the source is resolved. A description of how to convert from data values to physical units is provided in the LLORRI SIS document. 
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lucy:pivot_wavelength
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy:photometric_zero_point
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lucy:Diffuse_Source
      minimum occurrences   1
      maximum occurrences   1
      reference type        component_of

      local identifier      lucy:Point_Source
      minimum occurrences   1
      maximum occurrences   1
      reference type        component_of

End of Report
