PDS4 Local Data Dictionary Processing Report

Configuration:
   LDDTool Version        15.3.0
   LDD Version Id:        1.4.1.0
   LDD Label Version Id:  1.0
   LDD Discipline (T/F):  false
   LDD Namespace URL:     http://pds.nasa.gov/pds4/
   LDD URN Prefix:        urn:nasa:pds:
   Time                   Mon Aug 11 18:31:30 UTC 2025
   Common Schema          [PDS4_PDS_1O00.xsd]
   Common Schematron      [PDS4_PDS_1O00.sch]
   IM Version Id:         1.24.0.0
   IM Namespace Id:       pds
   IM Label Version Id:   1.0
   IM Object Model        [UpperModel.pont]
   IM Data Dictionary     [dd11179.pins]
   IM Glossary            [Glossary.pins]
   IM Document Spec       [DMDocument.pins]

Parameters:
   Input File             [/home/runner/work/ldd-mro/ldd-mro/src/PDS4_MRO_IngestLDD.xml]
   PDS Processing         true
   LDD Processing         true
   Discipline LDD         false
   Mission LDD            true
   Write Attr Elements    false
   Merge with Master      false

Summary:
   Classes                14
   Attributes             270
   Associations           284
   Error messages         0
   Warning messages       0
   Information messages   0

Detailed validation messages

Parsed Input - Header:
   LDD Name               MRO
   LDD Version            1.4.1.0
   Full Name              Jennifer Ward
   Steward                geo
   Namespace Id           mro
   Comment                
        The MRO dictionary contains classes that describe aspects of the 
        Mars Reconnaissance Orbiter mission and related instruments.
        
        MRO version 1.4.1.0
        PDS Build 1.19.0.0, 1.20.0.0, 1.21.0.0, 1.22.0.0, 1.23.0.0, 1.24.0.0
        LDDTool version 15.2.4
        
        Built with lddtool -plJ PDS4_MRO_IngestLDD.xml
        
        2022-09-27 JGW. Revised SCLK pattern to allow between 3 and 6 fractional digits.
        Added release_id.
        
        2022-09-29 JGW. Added SHARAD_Parameters class.
        Reorganized attribute definitions.
        
        2022-12-02 DVP. Added CRISM_ATO_Parameters class.
        
        2022-12-06 DVP. Bumped to version 1.1.0.0 because of addition of class.
	
	    2022-12-22 PG (pgeissler@usgs.gov) added HiRISE parameters, bumped to 1.2.0.0
	            
        2023-03-23 PG (pgeissler@usgs.gov) added HiRISE RDR class

	    2023-08-16 DVP. Modifications to some parameters of CRISM_ATO_Parameters class
	    following urn:nasa:pds:crism_ato_s_iof_lml peer review; bumped to 1.2.1.0

        2023-08-31 PG (pgeissler@usgs.gov) added observation_rationale attribute for HiRISE, 
        bump to 1.2.2.0
        
        2024-01-09 JGW. Added SHARAD_Observation_Parameters class, bump to 1.3.0.0
        
        2024-02-27 PG fixes to HiRISE, 1.3.1.0
        
        2024-09-16 JGW. Revised SCLK pattern to allow between 1 and 6 fractional digits, 1.3.2.0
        
        2025-12-16 TMH. Added BADCAL enumeration to special_processing_flag_* for HiRISE, 1.3.3.0
        
        2025-06-27 JGW. Added CRISM TRDR parameters. Added CRISM VRDR product types, 1.4.0.0
        
        2025-07-18 JGW. Added additional allowed values to mro:observation_type, 1.4.1.0 
        
    
   Last Modification Time 2025-06-27
   PDS4 Merge Flag        false

Parsed Input - Attributes:

   name                   mission_phase_name
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The mission_phase_name attribute provides the mission-defined name of a time period within the mission. 

   name                   observation_rationale
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The observation_rationale attribute identifies the name of the specific feature on Mars that was targeted by the observation. 

   name                   orbit_number
   version                1.24
   value data type        ASCII_NonNegative_Integer
   description             The orbit_number attribute identifies the orbit number when the observation was taken. 

   name                   producer_institution_name
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The producer_institution_name attribute identifies the name of the institution that created the data product. 

   name                   product_type
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The product_type attribute identifies the type of data product. 

   name                   product_version_id
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The product_version_id element identifies the version of an individual data product. 

   name                   release_id
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            release_id is the identifier of a scheduled release of MRO data from PDS. The first MRO data release has release_number "0001". The release_number for a given product is always the first release in which it appears, and does not change if the product is revised later.
   minimum characters     1

   name                   spacecraft_clock_count_partition
   version                1.24
   value data type        ASCII_NonNegative_Integer
   description             The spacecraft_clock_count_partition attribute indicates the clock partition active for the spacecraft_clock_start_count and spacecraft_clock_stop_count attributes. 

   name                   spacecraft_clock_start_count
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_start_count attribute provides the value of the spacecraft clock at the beginning of a time period of interest. 

   name                   spacecraft_clock_stop_count
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_stop_count attribute provides the value of the spacecraft clock at the end of a time period of interest. 

   name                   line_prefix_bytes
   version                1.24
   value data type        ASCII_NonNegative_Integer
   description             The line prefix bytes attribute reports the number of bytes that precede the observational data for each line of a HiRISE or CTX image. For HiRISE, the prefix includes 6 bytes of line identification information and the values of 12 buffer pixels, which contain the value of empty pixels after going through the instrument electronics. 

   name                   line_suffix_bytes
   version                1.24
   value data type        ASCII_NonNegative_Integer
   description             The line suffix bytes attribute reports the number of bytes that follow the observational data for each line of a HiRISE or CTX image. For HiRISE, the suffix contains 16 dark reference pixel values produced by masked detectors. 

   name                   activity_id
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The activity_id attribute describes the type of measurement contained in a CRISM EDR or other data product, and provides indication of how the observation is commanded. The format of the value is AC### where AC is a 2-letter designation of the type of measurement made, and ### is a 3-numeral designation of the instrument command macro that was executed to acquire the data. Macro numbers are in the range 0-255. For EDRs, BI is measurement of detector bias, DF is a measurement of background including dark current and thermal background, LP is measurement of a focal plane lamp, SP is measurement of the internal integrating sphere, and SC is measurement of an external scene. TP indicates that the EDR contains any test pattern produced by instrument electronics. T1 through T7 specify the test pattern, test pattern 1 through test pattern 7. UN indicates that the EDR contains data in which housekeeping does not match the commanded instrument configuration. For an RDR, RA indicates that the file contains values in units of radiance (W m^-2 nm^-1 sr^-1). IF indicates that the file contains values in units of I/F, or radiance divided by solar flux scaled for heliocentric distance. AL indicates that the file contains values as estimated Labert albedo, which is I/F corrected for cosine of incidence angle and for atmospheric and thermal effects. SU indicates that the files contains summary parameters, unitless values derived from Lambert albedo. For an RDR or a DDR, DE indicates that the files contains derived values related to observation geometry or independently characterized properties of the scene. 

   name                   band_name
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            Identifies the name of the CRISM band associated with the specific scaling and offset parameters used in a CRISM browse product. 

   name                   band_sequence_number
   version                1.24
   value data type        ASCII_Integer
   description            Defines the order of the CRISM bands along the Axis_Array when axis_name is band. 
   minimum value          1

   name                   detector_temperature
   version                1.24
   value data type        ASCII_Real
   description             The detector_temperature attribute provides the temperature of the CRISM IR detector (if sensor_id = 'L'), or the VNIR detector (if sensor_id = 'S'). On each detector there are two temperature sensors. The primary source of IR detector temperature is IR temperature sensor 1 (column 50 in the EDR list file). The backup source of IR detector temperature is IR temperature sensor 2 (column 51 in the EDR list file). The primary source of VNIR detector temperature is VNIR temperature sensor 2 (column 65 in the EDR list file). The backup source of VNIR detector temperature is VNIR temperature sensor 1 (column 64 in the EDR list file). 
   unit of measure type   Units_of_Temperature

   name                   exposure_parameter
   version                1.24
   value data type        ASCII_Integer
   description             The exposure_parameter attribute identifies the value supplied to the CRISM instrument to command the exposure time. At a given frame rate identified in frame_rate, there are 480 possible exposure times ranging from 1 to 480. An exposure parameter of 480 yields an exposure time equal to the inverse of the frame rate. An exposure time parameter of 1 yields an exposure time 1/480 as large. For example, at a frame rate of 3.75 Hz, an exposure time parameter of 480 yields an exposure time of 0.26667 sec, whereas an exposure time parameter of 1 yields and exposure time of 0.00056 sec. This parameter is included independently of the exposure time itself because some of the Calibration Data Records (CDRs) are applicable to data taken at a particular exposure parameter. 
   minimum value          1
   maximum value          480

   name                   fpe_temperature
   version                1.24
   value data type        ASCII_Real
   description             The fpe_temperature attribute provides the temperature of the HiRISE or CRISM instrument's Focal Plane Electronics in degrees Celsius. For HiRISE, see Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. For CRISM, the value refers to the focal plane electronics board mounted in the base of the gimbal. The values represents IR focal plane electronics if sensor_id = 'L', and to the VNIR focal plane electronics if sensor_id = 'S'. The source of CRISM IR focal plane electronics temperature is column 60 in the EDR list file. The source of VNIR focal plane electronics temperature is column 71 in the EDR list file. 
   unit of measure type   Units_of_Temperature

   name                   fram_stat_iqr_conf_lvl
   version                1.24
   value data type        ASCII_Real
   description             The fram_stat_iqr_conf_lvl attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the confidence level parameter associated with the Grubb's Test used for outlier detection of attributes of the normalized median profile of the frame interquartile range in the detection of bad frames during the preprocessing steps. Typical values are near 0.95. 
   minimum value          0
   maximum value          1

   name                   fram_stat_median_box_width
   version                1.24
   value data type        ASCII_Integer
   description             The fram_stat_median_box_width attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the kernel size of a median filter used on the frame median profile in the computation of bad frames during preprocessing steps. 

   name                   fram_stat_median_conf_lvl
   version                1.24
   value data type        ASCII_Real
   description             The fram_stat_median_conf_lvl attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the confidence level parameter associated with the Grubb's Test used for outlier detection of attributes of the normalized median frame profile in the detection of bad frames during the preprocessing steps. Typical values are near 0.95. 
   minimum value          0
   maximum value          1

   name                   fram_stat_min_deviation
   version                1.24
   value data type        ASCII_Real
   description             The fram_stat_min_deviation attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the minimum deviation from the mean of an attribute of the normalized frame median profile necessary to be classified as a bad frame during the preprocessing steps. 
   minimum value          0
   maximum value          1

   name                   frame_rate
   version                1.24
   value data type        ASCII_Real
   description             The frame_rate attribute identifies the rate at which frames of data in a CRISM EDR were returned. 
   unit of measure type   Units_of_Frame_Rate

   name                   hdf_software_version_id
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The hdf_software_version_id attribute indicates the version of the software used by the CRISM hyperspectral data filter application. 

   name                   hdf_software_name
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The hdf_software_name attribute provides the name of the CRISM hyperspectral data filter software used to process radiance TRDR data into I/F. 

   name                   if_max_value
   version                1.24
   value data type        ASCII_Real
   description             The if_max_value attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the maximum valid value in units of I/F. Values outside of the valid range of I/F values are ignored during preprocessing steps. 

   name                   if_min_value
   version                1.24
   value data type        ASCII_Real
   description             The if_min_value attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the minimum valid value in units of I/F. Values outside of the valid range of I/F values are ignored during preprocessing steps. 

   name                   ikf_confidence_level_r1
   version                1.24
   value data type        ASCII_Real
   description             The ikf_confidence_level_r1 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the confidence level parameter associated with the Grubb's Test used for outlier detection of attributes of the model residuals in the Iterative Kernel Filter procedure. Spectral region 1. Typical values are near 0.95. 
   nillable               true
   minimum value          0
   maximum value          1

   name                   ikf_confidence_level_r2
   version                1.24
   value data type        ASCII_Real
   description             The ikf_confidence_level_r2 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the confidence level parameter associated with the Grubb's Test used for outlier detection of attributes of the model residuals in the Iterative Kernel Filter procedure. Spectral region 2. Typical values are near 0.95. 
   nillable               true
   minimum value          0
   maximum value          1

   name                   ikf_kernel_size_x_r1
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_kernel_size_x_r1 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the size of the kernel in the X direction used in the Iterative Kernel Filter procedure. Spectral region 1. 
   nillable               true

   name                   ikf_kernel_size_x_r2
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_kernel_size_x_r2 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the size of the kernel in the X direction used in the Iterative Kernel Filter procedure. Spectral region 2. 
   nillable               true

   name                   ikf_kernel_size_y_r1
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_kernel_size_y_r1 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the size of the kernel in the Y direction used in the Iterative Kernel Filter procedure. Spectral region 1. 
   nillable               true

   name                   ikf_kernel_size_y_r2
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_kernel_size_y_r2 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the size of the kernel in the Y direction used in the Iterative Kernel Filter procedure. Spectral region 2. 
   nillable               true

   name                   ikf_kernel_size_z_r1
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_kernel_size_z_r1 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the size of the kernel in the Z direction used in the Iterative Kernel Filter procedure. Spectral region 1. 
   nillable               true

   name                   ikf_kernel_size_z_r2
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_kernel_size_z_r2 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the size of the kernel in the Z direction used in the Iterative Kernel Filter procedure. Spectral region 2. 
   nillable               true

   name                   ikf_model_order_x_r1
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_model_order_x_r1 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the dimensionality of the model in the X direction used in the Iterative Kernel Filter procedure. Spectral region 1. 
   nillable               true

   name                   ikf_model_order_x_r2
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_model_order_x_r2 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the dimensionality of the model in the X direction used in the Iterative Kernel Filter procedure. Spectral region 2. 
   nillable               true

   name                   ikf_model_order_y_r1
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_model_order_y_r1 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the dimensionality of the model in the Y direction used in the Iterative Kernel Filter procedure. Spectral region 1. 
   nillable               true

   name                   ikf_model_order_y_r2
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_model_order_y_r2 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the dimensionality of the model in the Y direction used in the Iterative Kernel Filter procedure. Spectral region 2. 
   nillable               true

   name                   ikf_model_order_z_r1
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_model_order_z_r1 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the dimensionality of the model in the Z direction used in the Iterative Kernel Filter procedure. Spectral region 1. 
   nillable               true

   name                   ikf_model_order_z_r2
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_model_order_z_r2 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the dimensionality of the model in the Z direction used in the Iterative Kernel Filter procedure. Spectral region 2. 
   nillable               true

   name                   ikf_num_regions
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_num_regions attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the number of spectral regions identified for the application of the Iterative Kernel Filter procedure. 
   nillable               true

   name                   ikf_start_channel_r1
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_start_channel_r1 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the first channel number for spectral region 1 of the Iterative Kernel Filter procedure. 
   nillable               true
   minimum value          0
   maximum value          437

   name                   ikf_start_channel_r2
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_start_channel_r2 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the first channel number for spectral region 2 of the Iterative Kernel Filter procedure. 
   nillable               true
   minimum value          0
   maximum value          437

   name                   ikf_stop_channel_r1
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_stop_channel_r1 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the last channel number for spectral region 1 of the Iterative Kernel Filter procedure. 
   nillable               true
   minimum value          0
   maximum value          437

   name                   ikf_stop_channel_r2
   version                1.24
   value data type        ASCII_Integer
   description             The ikf_stop_channel_r2 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the last channel number for spectral region 2 of the Iterative Kernel Filter procedure. 
   nillable               true
   minimum value          0
   maximum value          437

   name                   ikf_weighting_stddev_r1
   version                1.24
   value data type        ASCII_Real
   description             The ikf_weighting_stddev_r1 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the weighting parameter for the final model evaluation in the Iterative Kernel Filter procedure. Spectral region 1. 
   nillable               true

   name                   ikf_weighting_stddev_r2
   version                1.24
   value data type        ASCII_Real
   description             The ikf_weighting_stddev_r2 attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the weighting parameter for the final model evaluation in the Iterative Kernel Filter procedure. Spectral region 2. 
   nillable               true

   name                   instrument_pointing_mode
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The instrument_pointing_mode element identifies the pointing mode of the CRISM gimbal. 

   name                   inv_lookup_table_file_name
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The inv_lookup_table_file_name element identifies the name of the CRISM file that gives the 12-bit DN value replacing each 8-bit DN value if lossy compression was performed (if compression_type=8_BIT). The inverse lookup table file is a nine-column, 4095-row text file. Column 1 gives each 8-bit value, 0 through 255. Columns 2 through 9 give the 12-bit values that replace them if lookup tables 0 through 7, respectively, were selected for data acquisition. Lookup tables are selected on a line by line basis. Which table is used for each line is indicated in the pixel-processing descriptive file named in pixel_proc_file_name. 

   name                   log_xform_neg_clip_value
   version                1.24
   value data type        ASCII_Real
   description             The log_xform_neg_clip_value attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the value used for any negative I/F value in the log base 10 transform. This effectively represents the minimum possible pixel value for the Iterative Kernel Filter procedure. 
   nillable               true

   name                   observation_id
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The observation_id attribute is a 8-byte hexadecimal integer uniquely identifying the observation. 

   name                   observation_number
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The observation_number attribute gives the monotonically increasing ordinal counter of the EDRs generated for a particular CRISM observation_id. CRISM generates several EDRs for a given observation_id. 

   name                   observation_type
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The observation_type attribute identifies the general type of observation. 

   name                   optical_bench_temperature
   version                1.24
   value data type        ASCII_Real
   description             The optical_bench_temperature attribute provides the temperature of the CRISM optical bench. It is a backup to sphere_temperature for modeling the output radiance of the onboard integrating sphere as a function of sphere temperature. 
   unit of measure type   Units_of_Temperature

   name                   pixel_proc_file_name
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The pixel_proc_file_name attribute gives the name of the file that documents the CRISM onboard compression options selected. Onboard compression converts a 14- bit DN with a value of 0-16383 to a 12-bit- 0-4095 value or 8-bit 0-255 value for downlink. Corrections are done on a line by line basis. The pixel processing file is a 4- column, 480-row text file. The four attributes in each row are the row number, the gain correction performed, the offset correction performed, and the 12 to 8 bit lookup table used if lossy compression is performed. Both gain and offset corrections are always performed to convert 14-bit to 12-bit values prior to downlink. First the offset is subtracted from the 14-bit value. Then the difference is multiplied by the gain to shorten the result to a 12-bit value. If lossy compression is being performed (if compression_type = 8_BIT), then the 12- to 8-bit lookup table value gives the table in the file named by lookup_table_file_name that was used to convert the 12-bit value to an 8- bit value. 

   name                   refz_median_box_width
   version                1.24
   value data type        ASCII_Integer
   description             The refz_median_box_width attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the kernel size of a median filter used in the spectral direction in the computation of the reference cube during the preprocessing steps. 

   name                   refz_smooth_box_width
   version                1.24
   value data type        ASCII_Integer
   description             The refz_smooth_box_width attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the kernel size of a boxcar smoothing filter used in the spectral direction in the computation of the reference cube during the preprocessing steps. 

   name                   rsc_ref_xy_median_width
   version                1.24
   value data type        ASCII_Integer
   description             The rsc_ref_xy_median_width attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the kernel size of a median filter used as part of the application of the ratio shift correction procedure in the XY direction while computing the reference cube during the preprocessing steps. 

   name                   rsc_ref_xy_smooth_width
   version                1.24
   value data type        ASCII_Integer
   description             The rsc_ref_xy_smooth_width attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the kernel size of a boxcar smoothing filter used as part of the application of the ratio shift correction procedure in the XY direction while computing the reference cube during the preprocessing steps. 

   name                   rsc_ref_yz_median_width
   version                1.24
   value data type        ASCII_Integer
   description             The rsc_ref_yz_median_width attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the kernel size of a median filter used as part of the application of the ratio shift correction procedure in the YZ direction while computing the reference cube during the preprocessing steps. 

   name                   rsc_ref_yz_smooth_width
   version                1.24
   value data type        ASCII_Integer
   description             The rsc_ref_yz_smooth_width attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the kernel size of a boxcar smoothing filter used as part of the application of the ratio shift correction procedure in the YZ direction while computing the reference cube during the preprocessing steps. 

   name                   rsc_ratio_xy_median_width
   version                1.24
   value data type        ASCII_Integer
   description             The rsc_ratio_xy_median_width attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the kernel size of a median filter used as part of the application of the ratio shift correction procedure in the XY direction while computing the ratio cube during the preprocessing steps. 

   name                   rsc_ratio_xy_smooth_width
   version                1.24
   value data type        ASCII_Integer
   description             The rsc_ratio_xy_smooth_width attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the kernel size of a boxcar smoothing filter used as part of the application of the ratio shift correction procedure in the XY direction while computing the ratio cube during the preprocessing steps. 

   name                   rsc_res_xy_ply_order
   version                1.24
   value data type        ASCII_Integer
   description             The rsc_res_xy_ply_order attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the order of the polynomial used to model low frequency content in the XY direction used as part of the application of the ratio shift correction procedure while computing the resolve cube during the post processing steps. 

   name                   rsc_res_xy_ply_extnd_width
   version                1.24
   value data type        ASCII_Integer
   description             The rsc_res_xy_ply_extnd_width attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the number of pixels used to extend the trend of the column profiles when computing the polynomial used to model low frequency content in the XY direction used as part of the application of the ratio shift correction procedure while computing the resolve cube during the post processing steps. 

   name                   sampling_mode_id
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The sampling_mode_id attribute identifies the resolution mode of a wavelength or frequency channel. 

   name                   scaling_factor
   version                1.24
   value data type        ASCII_Real
   description            The scaling_factor attribute is the scaling factor to be applied to each stored value in order to recover an original value. The observed value (Ov) is calculated from the stored value (Sv) thus: Ov = (Sv * scaling_factor) + value_offset. 

   name                   scan_mode_id
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The scan_mode_id attribute identifies one of several internal rates for data acquisition by an instrument. 

   name                   sensor_id
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The sensor_id attribute identifies the CRISM focal plane from which data in an EDR or RDR were returned; S = short-wavelength or VNIR, L = long-wavelength or IR, J = joint where a data product is applicable to either. 

   name                   spectrometer_housing_temperature
   version                1.24
   value data type        ASCII_Real
   description             The spectrometer_housing_temperature attribute gives the temperature of the CRISM spectrometer housing. This is a backup to direct determination, using measurements with the shutter closed, of the thermal background measured by the IR detector. The primary source of this temperature is a measurement digitized by the VNIR focal plane electronics, column 58 in the EDR list file. The backup source of this temperature is a measurement digitized by the IR focal plane electronics, column 69 in the EDR list file. 
   unit of measure type   Units_of_Temperature

   name                   sphere_temperature
   version                1.24
   value data type        ASCII_Real
   description             The sphere_temperature attribute gives the temperature of the CRISM onboard integrating sphere. It is used for modeling the output radiance of the sphere as a function of sphere temperature. 
   unit of measure type   Units_of_Temperature

   name                   trace_max_value
   version                1.24
   value data type        ASCII_Real
   description            The trace_max_value attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the maximum valid value of a ratio computed for the Ratio Shift Correction algorithm. Values outside of the valid range of ratio values are ignored during this processing steps. 

   name                   trace_min_value
   version                1.24
   value data type        ASCII_Real
   description            The trace_min_value attribute is one of the control parameters for the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F and indicates the minimum valid value of a ratio computed for the Ratio Shift Correction algorithm. Values outside of the valid range of ratio values are ignored during this processing steps. 

   name                   value_offset
   version                1.24
   value data type        ASCII_Real
   description            The value_offset attribute is the offset to be applied to each stored value in order to recover an original value. The observed value (Ov) is calculated from the stored value (Sv) thus: Ov = (Sv * scaling_factor) + value_offset. 

   name                   wavelength_file_name
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The wavelenth_file_name attribute identifies the name of the file that describes wavelength sampling in a CRISM EDR, RDR, or CDR. There are two aspects to the wavelength sampling. One is the wavelength of light falling on each attribute of the 480-row detector. The second is the selection of which rows are included in downlink. For each detector there is a menu of four options; which option is selected is given in wavelength_filter, which has a value of 0, 1, 2, or 3. For an EDR, the wavelength file is a 5-column, 480-row text file. The five attributes in each row are the row number and a 0 or 1 for wavelength_filter 0, 1, 2 and 3, indicating if the row is included in the EDR when that option is selected in wavelength_filter. For an RDR or CDR, the wavelength file is an image whose value at the location of a detector attribute is the center wavelength of that attribute, in nanometers. 

   name                   wavelength_filter
   version                1.24
   value data type        ASCII_Integer
   description            The wavelength_filter attribute identifies which of four CRISM onboard menus of rows was selected for downlink. The four choices are 0, 1, 2, or 3. Each filter is a vector of 480 0's or 1's, one per row of the detector. 0 indicates that data are not saved; 1 indicates that data are saved. The values in the four vectors are in the file named by wavelength_file_name. 

   name                   array_first_value
   version                1.24
   value data type        ASCII_Real
   description            The array_first_value element provides the first value in an ascending series and is therefore the minimum value at which a given data item was sampled. 

   name                   array_interval
   version                1.24
   value data type        ASCII_Real
   description            The array_interval attribute provides the spacing of points at which data are sampled and at which values for an instrument or other parameter are available. If x1 and xn are the first and last sampling parameter values, respectively, xn is larger than x1, n is the number of sampling parameters, the caret symbol (^) denotes exponentiation, and b, a positive real number, is the base for exponentiation, then the value of sampling_parameter_interval is: (xn-x1)/(n-1) (for sampling_parameter_scale = Linear), (xn/x1)^(1/(n-1)) (for sampling_parameter_scale = Logarithmic), (b^xn-b^x1)/(n-1) (for sampling_parameter_scale = Exponential). 

   name                   array_last_value
   version                1.24
   value data type        ASCII_Real
   description            The array_last_value element provides the last value in an ascending series and is therefore the maximum value at which a given data item was sampled. 

   name                   array_scale
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The array_scale attribute specifies whether the sampling interval is linear or something other such as logarithmic. 

   name                   array_unit
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The array_unit element specifies the unit of measure of associated data sampling parameters. 

   name                   azimuth_processing_window
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The windowing function used to reduce sidelobes resulting from azimuth (along-track) synthetic aperture processing of the raw echo records. All radargrams in the SHARAD radargram archive use a Hann function. 

   name                   chirp_frequency_envelope
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The frequency-dependent amplitude variation used in range compression of the raw echo data. All radargrams in the SHARAD radargram archive use a uniform-amplitude model. 

   name                   multilook_doppler_bandwidth
   version                1.24
   value data type        ASCII_Real
   description            The frequency span over which radar echoes are averaged, following synthetic aperture processing for each spatial footprint along the ground track. This frequency span is measured to either side of the zero-frequency component of the Doppler spectrum. 
   unit of measure type   Units_of_Frequency

   name                   name
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The name element provides the name of the parameter which determines the sampling interval of a particular instrument or dataset parameter. For example, magnetic field intensity is sampled in time increments, and a spectrum is sampled in wavelength or frequency. 

   name                   number_of_looks
   version                1.24
   value data type        ASCII_Integer
   description            The number of frequency-resolved cells included in the multi-look averaging. This varies with the chosen frequency span and the Doppler resolution set by the inverse of the coherent integration time. 

   name                   range_compression_window
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The windowing function used to reduce sidelobes resulting from range compression of the raw echo records. All radargrams in the SHARAD radargram archive use a Hann function. 

   name                   synthetic_aperture_duration
   version                1.24
   value data type        ASCII_Real
   description            The coherent integration time for SHARAD signals processed using the synthetic aperture technique. Multiplication of this value by the MRO tangential velocity tabulated in the SHARAD radargram *GEOM.TAB files yields an approximate physical length of the aperture. 
   unit of measure type   Units_of_Time

   name                   max_sample
   version                1.24
   value data type        ASCII_Integer
   description            The index of the highest-numbered sample/column of this product relative to the original CRISM scene. The first sample of the original CRISM scene corresponds to a value of 1. 

   name                   max_line
   version                1.24
   value data type        ASCII_Integer
   description            The index of the highest-numbered line/row of this product relative to the original CRISM scene. The first line of the original CRISM scene corresponds to a value of 1. 

   name                   min_sample
   version                1.24
   value data type        ASCII_Integer
   description            The index of the lowest-numbered sample/column of this product relative to the original CRISM scene. The first sample of the original CRISM scene corresponds to a value of 1. 

   name                   min_line
   version                1.24
   value data type        ASCII_Integer
   description            The index of the lowest-numbered line/row of this product relative to the original CRISM scene. The first line of the original CRISM scene corresponds to a value of 1. 

   name                   analog_power_start_count
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The analog_power_start_count attribute provides the spacecraft clock count when power to the CPMM units was applied. 

   name                   analog_power_start_time
   version                1.24
   value data type        ASCII_Date_Time_YMD_UTC
   description             The analog_power_start_time attribute provides the UTC time when power to the CPMM units was applied. 

   name                   calibration_start_count
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The calibration_start_count attribute provides the spacecraft clock count at the beginning of the first calibration image line. 

   name                   calibration_start_time
   version                1.24
   value data type        ASCII_Date_Time_YMD_UTC
   description             The calibration_start_time attribute provides the UTC time at the beginning of the first calibration image line. 

   name                   observation_start_time
   version                1.24
   value data type        ASCII_Date_Time_YMD_UTC
   description             The observation_start_time attribute provides the UTC start time of a HiRISE image acquisition sequence. 

   name                   readout_start_count
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The readout_start_count attribute provides the spacecraft clock count when the HiRISE CCD Process/Memory Module begins transferring image data out of its buffer memory. 

   name                   readout_start_time
   version                1.24
   value data type        ASCII_Date_Time_YMD_UTC
   description             The readout_start_time attribute provides the UTC time when the HiRISE CCD Process/Memory Module begins transferring image data out of buffer memory. 

   name                   adc_timing_settings_image
   version                1.24
   value data type        ASCII_Integer
   description             The adc_timing_settings_image attribute provides the HiRISE Channel 0 analog-to-digital conversion timing settings for the readout of the video waveform. 
   minimum value          0
   maximum value          9

   name                   adc_timing_settings_reset
   version                1.24
   value data type        ASCII_Integer
   description             The adc_timing_settings_reset attribute provides the HiRISE Channel 0 analog-to-digital conversion timing settings for the reset of the video waveform. 
   minimum value          0
   maximum value          9

   name                   binning
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 

   name                   channel_number
   version                1.24
   value data type        ASCII_Integer
   description             The channel_number attribute provides the HiRISE CCD channel number. 

   name                   cpmm_number
   version                1.24
   value data type        ASCII_Integer
   description             The cpmm_number attribute provides the HiRISE CCD Processing/Memory Module number. 

   name                   delta_line_timer_count
   version                1.24
   value data type        ASCII_Real
   description             The delta_line_timer_count element provides the commanded count given to the HiRISE instrument to set the scan line duration. mro:scan_line_duration = 74 + mro:delta_line_timer_count/16 
   minimum value          0
   maximum value          16777216

   name                   dll_frequency_correct_count
   version                1.24
   value data type        ASCII_Integer
   description             The dll_frequency_correct_count attribute provides a count of the number of times the HiRISE 96 MHz clock frequency was observed to be correct. This is used with the recursive Digital Lock Loop reset circuit. 
   minimum value          0
   maximum value          255

   name                   dll_locked_flag_01
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The dll_locked_flag_01 attribute provides the state of the 1st 96 Mhz Digital Lock Loop flag for a HiRISE observation. 

   name                   dll_locked_flag_02
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The dll_locked_flag_02 attribute provides the state of the 2nd 96 Mhz Digital Lock Loop flag for a HiRISE observation. 

   name                   dll_locked_once_flag_01
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The dll_locked_once_flag_01 attribute indicates if the 1st Digital Lock Loop ever locked during a HiRISE observation. 

   name                   dll_locked_once_flag_02
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The dll_locked_once_flag_02 attribute indicates if the 2nd Digital Lock Loop ever locked during a HiRISE observation. 

   name                   dll_reset_count
   version                1.24
   value data type        ASCII_Integer
   description             The dll_reset_count attribute provides the count of the number of times during a HiRISE observation the 96 MHz Digital Lock Loop had to be reset in order to lock to the incoming 48 Mhz clock and produce an 96 MHz clock. 
   minimum value          0
   maximum value          255

   name                   felics_compression_flag
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The felics_compression_flag element identifies whether FELICS data compression was applied to a HiRISE image. 

   name                   focus_position_count
   version                1.24
   value data type        ASCII_Real
   description             The focus_position_count attribute provides the raw count of the focus mechanism position in a HiRISE observation. 

   name                   heater_control_flag_00
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_flag_01
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_flag_02
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_flag_03
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_flag_04
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_flag_05
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_flag_06
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_flag_07
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_flag_08
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_flag_09
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_flag_10
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_flag_11
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_flag_12
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_flag_13
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_flag element is a set of 14 on/off flags that indicate which of the 14 heater control areas were on at the time of a HiRISE observation. 

   name                   heater_control_mode
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The heater_control_mode attribute provides the state of the HiRISE heater control, either closed-loop or duty-cycle. Normally the closed-loop mode is used to keep nominal operating temperatures of the instrument. A duty-cycle mode is enabled during periods of high EM emissions from other MRO instruments. 

   name                   image_exposure_duration
   version                1.24
   value data type        ASCII_Real
   description             The image_exposure_duration attribute provides the total time of a HiRISE observation from the start of the first line to the end of the last line computed by multiplying the total number of lines in the array times the line exposure duration. Units of microseconds. 
   unit of measure type   Units_of_Time

   name                   line_exposure_duration
   version                1.24
   value data type        ASCII_Real
   description             The line_exposure_duration attribute provides the time from the start of exposure of one binned line to the start of exposure of the next binned line in a HiRISE image. Units of microseconds. 
   unit of measure type   Units_of_Time

   name                   lookup_table_k_value
   version                1.24
   value data type        ASCII_Integer
   description             The lookup_table_k_value attribute provides the 'pixel spread' value in a HiRISE image. This parameter is used only for the HiRISE SQUARE-ROOT LUT table mode. A -9998 value indicates a K value was not used. 
   minimum value          -9998
   maximum value          32

   name                   lookup_table_maximum
   version                1.24
   value data type        ASCII_Integer
   description             The lookup_table_maximum attribute provides the maximum 14-bit pixel value mapped to the 254 DN 8-bit pixel in a HiRISE image. This parameter is used only for the HiRISE LINEAR LUT table mode. A -9998 value indicates that the maximum value was not used. 
   minimum value          -9998
   maximum value          16384

   name                   lookup_table_median
   version                1.24
   value data type        ASCII_Integer
   description             The lookup_table_median attribute provides the median 14-bit pixel value mapped to the 254 DN 8-bit pixel in a HiRISE image. This parameter is used only for the HiRISE SQUARE-ROOT LUT table mode. A -9998 value indicates that the table median value was not used. 
   minimum value          -9998
   maximum value          16384

   name                   lookup_table_minimum
   version                1.24
   value data type        ASCII_Integer
   description             The lookup_table_minimum attribute provides the minimum 14-bit pixel value mapped to the 0 DN output pixel in a HiRISE image. This parameter is used only for the HiRISE LINEAR LUT table mode. A -9998 value indicates that the maximum value was not used. 
   minimum value          -9998
   maximum value          16384

   name                   lookup_table_number
   version                1.24
   value data type        ASCII_Integer
   description             The lookup_table_number attribute provides the number of the stored LUT used in a HiRISE image. This parameter is used only for the HiRISE STORED LUT table mode. A value of -9998 indicates that a table number was not used. 
   minimum value          -9998
   maximum value          28

   name                   lookup_table_type
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The lookup_table_type attribute provides the type of lookup table that was applied to convert 14-bit pixels to 8-bit pixels in a HiRISE image. 

   name                   powered_cpmm_flag_00
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   powered_cpmm_flag_01
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   powered_cpmm_flag_02
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   powered_cpmm_flag_03
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   powered_cpmm_flag_04
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   powered_cpmm_flag_05
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   powered_cpmm_flag_06
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   powered_cpmm_flag_07
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   powered_cpmm_flag_08
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   powered_cpmm_flag_09
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   powered_cpmm_flag_10
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   powered_cpmm_flag_11
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   powered_cpmm_flag_12
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   powered_cpmm_flag_13
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The powered_cpmm_flag attribute provides a set of 14 values that identify which HiRISE CCD Processing/Memory Modules were commanded to acquire imaging during the observation. The first element is for CPMM 0 and the last element is for CPMM 13. 

   name                   scan_exposure_duration
   version                1.24
   value data type        ASCII_Real
   description             The scan_exposure_duration attribute provides the unbinned line readout rate of the HiRISE instrument in microseconds. This corresponds to the time between successive steps in the Time Delay Integration (TDI) process. The adjustment of this parameter is used to match image line acquisition to the boresight ground velocity. The value is the same for all CCDs for a given observation. 
   minimum value          74
   maximum value          1048650
   unit of measure type   Units_of_Time

   name                   stimulation_lamp_flag_red
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The stimulation_lamp_flag attribute is a set of three flags that identify which of the three HiRISE stimulation lamps have been turned on or off. Stimulation lamps are used to evaluate relative changes in instrument calibration throughout the mission. Stimulation lamps are always turned off for science observation data. 

   name                   stimulation_lamp_flag_nir
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The stimulation_lamp_flag attribute is a set of three flags that identify which of the three HiRISE stimulation lamps have been turned on or off. Stimulation lamps are used to evaluate relative changes in instrument calibration throughout the mission. Stimulation lamps are always turned off for science observation data. 

   name                   stimulation_lamp_flag_blg
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The stimulation_lamp_flag attribute is a set of three flags that identify which of the three HiRISE stimulation lamps have been turned on or off. Stimulation lamps are used to evaluate relative changes in instrument calibration throughout the mission. Stimulation lamps are always turned off for science observation data. 

   name                   tdi
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 

   name                   trim_lines
   version                1.24
   value data type        ASCII_Integer
   description             The trim_lines attribute provides the number of lines that have been trimmed at the beginning of a HiRISE observation. 
   minimum value          0

   name                   barrel_baffle_temperature
   version                1.24
   value data type        ASCII_Real
   description             The barrel_baffle_temperature attribute provides the temperature of the HiRISE instrument's barrel baffle in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   cpmm_pws_board_temperature
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_pws_board_temperature attribute provides the temperature of the HiRISE instrument's CCD Processing/Memory Module Power Supply Board in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   field_stop_temperature
   version                1.24
   value data type        ASCII_Real
   description             The field_stop_temperature attribute provides the temperature of the HiRISE instrument's focus mechanism field stop in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   focus_motor_temperature
   version                1.24
   value data type        ASCII_Real
   description             The focus_motor_temperature attribute provides the temperature of the HiRISE instrument's focus mirror in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   fpa_negative_y_temperature
   version                1.24
   value data type        ASCII_Real
   description             The fpa_negative_y_temperature attribute provides the temperature of the HiRISE instrument's Focal Plane Array -Y location in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   fpa_positive_y_temperature
   version                1.24
   value data type        ASCII_Real
   description             The fpa_positive_y_temperature attribute provides the temperature of the HiRISE instrument's Focal Plane Array +Y side location in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   iea_temperature
   version                1.24
   value data type        ASCII_Real
   description             The iea_temperature attribute provides the temperature of the HiRISE instrument's Instrument Electronics Assembly in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   ie_pws_board_temperature
   version                1.24
   value data type        ASCII_Real
   description             The ie_pws_board_temperature attribute provides the temperature of the HiRISE instrument's Instrument Electronics Power Supply Board in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   inst_cont_board_temperature
   version                1.24
   value data type        ASCII_Real
   description             The inst_cont_board_temperature attribute provides the temperature of the HiRISE instrument control board in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   mech_tlm_board_temperature
   version                1.24
   value data type        ASCII_Real
   description             The mech_tlm_board_temperature attribute provides the temperature of the HiRISE instrument's Mech/TLM Board in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   ms_truss_leg_0_a_temperature
   version                1.24
   value data type        ASCII_Real
   description             The ms_truss_leg_0_a_temperature attribute provides the temperature of the HiRISE instrument's metering structure truss 0-A leg in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   ms_truss_leg_0_b_temperature
   version                1.24
   value data type        ASCII_Real
   description             The ms_truss_leg_0_b_temperature attribute provides the temperature of the HiRISE instrument's metering structure truss 0-B leg in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   ms_truss_leg_120_a_temperature
   version                1.24
   value data type        ASCII_Real
   description             The ms_truss_leg_120_a_temperature attribute provides the temperature of the HiRISE instrument's metering structure truss 120-A leg in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   ms_truss_leg_120_b_temperature
   version                1.24
   value data type        ASCII_Real
   description             The ms_truss_leg_120_b_temperature attribute provides the temperature of the HiRISE instrument's metering structure truss 120-B leg in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   ms_truss_leg_240_a_temperature
   version                1.24
   value data type        ASCII_Real
   description             The ms_truss_leg_240_a_temperature attribute provides the temperature of the HiRISE instrument's metering structure truss 240-A leg in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   ms_truss_leg_240_b_temperature
   version                1.24
   value data type        ASCII_Real
   description             The ms_truss_leg_240_b_temperature attribute provides the temperature of the HiRISE instrument's metering structure truss 240-B leg in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   opt_bnch_box_beam_temperature
   version                1.24
   value data type        ASCII_Real
   description             The opt_bnch_box_beam_temperature attribute provides the temperature of the HiRISE instrument's optical bench near the box beam (+Y face) in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   opt_bnch_cover_temperature
   version                1.24
   value data type        ASCII_Real
   description             The opt_bnch_cover_temperature attribute provides the temperature of the HiRISE instrument's optical bench cover (external) in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   opt_bnch_flexure_temperature
   version                1.24
   value data type        ASCII_Real
   description             The opt_bnch_flexure_temperature attribute provides the temperature of the HiRISE instrument's optical bench near the +X MDR flexure in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   opt_bnch_fold_flat_temperature
   version                1.24
   value data type        ASCII_Real
   description             The opt_bnch_fold_flat_temperature attribute provides the temperature of the HiRISE instrument's optical fold flat mirror location in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   opt_bnch_fpa_temperature
   version                1.24
   value data type        ASCII_Real
   description             The opt_bnch_fpa_temperature attribute provides the temperature of the HiRISE instrument's optical bench near the Focal Plane Array in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   opt_bnch_fpe_temperature
   version                1.24
   value data type        ASCII_Real
   description             The opt_bnch_fpe_temperature attribute provides the temperature of the HiRISE instrument's optical bench near the Focal Plane Electronics in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   opt_bnch_living_rm_temperature
   version                1.24
   value data type        ASCII_Real
   description             The opt_bnch_living_rm_temperature attribute provides the temperature of the HiRISE instrument's optical bench in the sunken living room location in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   opt_bnch_mirror_temperature
   version                1.24
   value data type        ASCII_Real
   description             The opt_bnch_mirror_temperature attribute provides the temperature of the HiRISE instrument's optical bench near the tertiary mirror in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   primary_mirror_baf_temperature
   version                1.24
   value data type        ASCII_Real
   description             The primary_mirror_baf_temperature attribute provides the temperature of the HiRISE instrument's primary mirror baffle near the base (external) in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   primary_mirror_mnt_temperature
   version                1.24
   value data type        ASCII_Real
   description             The primary_mirror_mnt_temperature attribute provides the temperature of the HiRISE instrument's primary mirror mount in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   primary_mirror_temperature
   version                1.24
   value data type        ASCII_Real
   description             The primary_mirror_temperature attribute provides the temperature of the HiRISE instrument's primary mirror at its maximum thickness in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   sec_mirror_baffle_temperature
   version                1.24
   value data type        ASCII_Real
   description             The sec_mirror_baffle_temperature attribute provides the temperature of the HiRISE instrument's secondary mirror baffle near the base (external) in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   sec_mirror_mtr_rng_temperature
   version                1.24
   value data type        ASCII_Real
   description             The sec_mirror_mtr_rng_temperature attribute provides the temperature of the HiRISE instrument's secondary mirror metering ring in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   sec_mirror_temperature
   version                1.24
   value data type        ASCII_Real
   description             The sec_mirror_temperature attribute provides the temperature of the HiRISE instrument's secondary mirror in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   spider_leg_150_temperature
   version                1.24
   value data type        ASCII_Real
   description             The spider_leg_150_temperature attribute provides the temperature of the HiRISE instrument's spider leg at the 150 degree location in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   spider_leg_270_temperature
   version                1.24
   value data type        ASCII_Real
   description             The spider_leg_270_temperature attribute provides the temperature of the HiRISE instrument's spider leg at the 270 degree location in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   spider_leg_30_temperature
   version                1.24
   value data type        ASCII_Real
   description             The spider_leg_30_temperature attribute provides the temperature of the HiRISE instrument's spider leg at the 30 degree location in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   sun_shade_temperature
   version                1.24
   value data type        ASCII_Real
   description             The sun_shade_temperature attribute provides the temperature of the HiRISE instrument's sun shade under the MLI in degrees Centigrade. See Figure 2.3, MRO HiRISE EDR SIS, REFKEYID JPLD-32004. 
   unit of measure type   Units_of_Temperature

   name                   cpmm_negative_5_current
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_negative_5_current attribute provides the negative 5 current of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Current

   name                   cpmm_negative_5_voltage
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_negative_5_voltage attribute provides the negative 5 voltage state of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Voltage

   name                   cpmm_positive_10_current
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_positive_10_current attribute provides the positive 10 current of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Current

   name                   cpmm_positive_10_voltage
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_positive_10_voltage attribute provides the positive 10 voltage state of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Voltage

   name                   cpmm_positive_1_8_current
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_positive_1_8_current attribute provides the positive 1_8 current of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Current

   name                   cpmm_positive_1_8_voltage
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_positive_1_8_voltage attribute provides the positive 1_8 voltage state of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Voltage

   name                   cpmm_positive_2_5_current
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_positive_2_5_current attribute provides the positive 2_5 current of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Current

   name                   cpmm_positive_2_5_voltage
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_positive_2_5_voltage attribute provides the positive 2_5 voltage state of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Voltage

   name                   cpmm_positive_29_current
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_positive_29_current attribute provides the positive 29 current of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Current

   name                   cpmm_positive_29_voltage
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_positive_29_voltage attribute provides the positive 29 voltage state of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Voltage

   name                   cpmm_positive_3_3_current
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_positive_3_3_current attribute provides the positive 3_3 current of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Current

   name                   cpmm_positive_3_3_voltage
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_positive_3_3_voltage attribute provides the positive 3_3 voltage state of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Voltage

   name                   cpmm_positive_5_current
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_positive_5_current attribute provides the positive 5 current of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Current

   name                   cpmm_positive_5_voltage
   version                1.24
   value data type        ASCII_Real
   description             The cpmm_positive_5_voltage attribute provides the positive 5 voltage state of the HiRISE CCD Processing/Memory Module. 
   unit of measure type   Units_of_Voltage

   name                   heater_current
   version                1.24
   value data type        ASCII_Real
   description             The heater_current attribute provides the HiRISE heater current in amps. 
   unit of measure type   Units_of_Current

   name                   iea_negative_15_voltage
   version                1.24
   value data type        ASCII_Real
   description             The iea_negative_15_voltage attribute provides the negative 15 voltage state of the HiRISE Interface Electronics Assembly. 
   unit of measure type   Units_of_Voltage

   name                   iea_positive_15_voltage
   version                1.24
   value data type        ASCII_Real
   description             The iea_positive_15_voltage attribute provides the positive 15 voltage state of the HiRISE Interface Electronics Assembly. 
   unit of measure type   Units_of_Voltage

   name                   iea_positive_28_voltage
   version                1.24
   value data type        ASCII_Real
   description             The iea_positive_28_voltage attribute provides the positive 28 voltage state of the HiRISE Interface Electronics Assembly. 
   unit of measure type   Units_of_Voltage

   name                   iea_positive_5_voltage
   version                1.24
   value data type        ASCII_Real
   description             The iea_positive_5_voltage attribute provides the positive 5 voltage state of the HiRISE Interface Electronics Assembly. 
   unit of measure type   Units_of_Voltage

   name                   inst_cont_fpga_pos_2_5_voltage
   version                1.24
   value data type        ASCII_Real
   description             The inst_cont_fpga_pos_2_5_voltage attribute provides the positive 2_5 voltage state of the HiRISE instrument control Field-Programmable Gate Array. 
   unit of measure type   Units_of_Voltage

   name                   mech_tlm_fpga_pos_2_5_voltage
   version                1.24
   value data type        ASCII_Real
   description             The mech_tlm_fpga_pos_2_5_voltage attribute provides the positive 2_5 voltage state of the HiRISE Mech/TLM Field-Programmable Gate Array. 
   unit of measure type   Units_of_Voltage

   name                   binning_red0
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   binning_red1
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   binning_red2
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   binning_red3
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   binning_red4
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   binning_red5
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   binning_red6
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   binning_red7
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   binning_red8
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   binning_red9
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   binning_ir10
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   binning_ir11
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   binning_bg12
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   binning_bg13
   version                1.24
   value data type        ASCII_Integer
   description             The binning element provides the HiRISE observation binning mode; i.e., the number of lines binned in an observation. mro:line_exposure_duration = mro:binning * mro:scan_line_duration 
   nillable               true

   name                   ccd_flag_red0
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   ccd_flag_red1
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   ccd_flag_red2
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   ccd_flag_red3
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   ccd_flag_red4
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   ccd_flag_red5
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   ccd_flag_red6
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   ccd_flag_red7
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   ccd_flag_red8
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   ccd_flag_red9
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   ccd_flag_ir10
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   ccd_flag_ir11
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   ccd_flag_bg12
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   ccd_flag_bg13
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The ccd_flag elements identify which CCDs were operating at the time of an observation. There is a special processing flag for each CCD used in the observation. 

   name                   maximum_stretch
   version                1.24
   value data type        ASCII_Integer
   description             The maximum_stretch attribute provides a contrast stretch value to be used in the display of a HiRISE Image. The mro.maximum_stretch parameter specifies the DN value to map to the 255 DN value of the display. For color images, there will be three values, one for each color. 
   minimum value          0
   maximum value          1024

   name                   minimum_stretch
   version                1.24
   value data type        ASCII_Integer
   description             The minimum_stretch attribute provides a contrast stretch value to be used in the display of a HiRISE Image. The mro.minimum_stretch parameter specifies the DN value to map to the 0 DN value of the display. For color images, there will be three values, one for each color. 
   minimum value          0
   maximum value          1024

   name                   special_processing_flag_red0
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   special_processing_flag_red1
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   special_processing_flag_red2
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   special_processing_flag_red3
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   special_processing_flag_red4
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   special_processing_flag_red5
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   special_processing_flag_red6
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   special_processing_flag_red7
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   special_processing_flag_red8
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   special_processing_flag_red9
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   special_processing_flag_ir10
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   special_processing_flag_ir11
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   special_processing_flag_bg12
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   special_processing_flag_bg13
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description             The special_processing_flag elements indicate if special calibration processing was applied to a HiRISE CCD image. The HiRISE instrument may experience instability problems or a low-signal image may have been poorly calibrated requiring an alternate calibration strategy. There is a special processing flag for each CCD used in the observation. 

   name                   tdi_red0
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

   name                   tdi_red1
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

   name                   tdi_red2
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

   name                   tdi_red3
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

   name                   tdi_red4
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

   name                   tdi_red5
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

   name                   tdi_red6
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

   name                   tdi_red7
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

   name                   tdi_red8
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

   name                   tdi_red9
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

   name                   tdi_ir10
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

   name                   tdi_ir11
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

   name                   tdi_bg12
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

   name                   tdi_bg13
   version                1.24
   value data type        ASCII_Integer
   description             The tdi attribute provides the number of time delay and integration (TDI) stages used to increase the exposure time of a HiRISE observation. 
   nillable               true

Parsed Input - Classes:

   name                   HiRISE_Time_Parameters
   description            The HiRISE_Time_Parameters class contains attributes specific to HiRISE EDRs.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.observation_start_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.readout_start_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.readout_start_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.analog_power_start_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.analog_power_start_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.calibration_start_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.calibration_start_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   HiRISE_Instrument_Setting_Parameters
   description            The HiRISE_Instrument_Setting_Parameters class contains attributes specific to HiRISE EDRs.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.cpmm_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.channel_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.scan_exposure_duration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.line_exposure_duration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.image_exposure_duration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.delta_line_timer_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_00
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_01
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_02
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_03
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_04
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_05
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_06
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_07
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_08
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_09
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_10
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_11
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_12
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.powered_cpmm_flag_13
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.trim_lines
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.focus_position_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.felics_compression_flag
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.stimulation_lamp_flag_red
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.stimulation_lamp_flag_blg
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.stimulation_lamp_flag_nir
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_mode
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_00
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_01
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_02
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_03
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_04
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_05
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_06
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_07
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_08
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_09
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_10
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_11
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_12
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_control_flag_13
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.lookup_table_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.lookup_table_minimum
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.lookup_table_maximum
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.lookup_table_median
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.lookup_table_k_value
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.lookup_table_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.adc_timing_settings_image
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.adc_timing_settings_reset
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.dll_locked_flag_01
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.dll_locked_flag_02
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.dll_locked_once_flag_01
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.dll_locked_once_flag_02
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.dll_reset_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.dll_frequency_correct_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   HiRISE_Temperature_Parameters
   description            The HiRISE_Temperature_Parameters class contains attributes specific to HiRISE EDRs.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.opt_bnch_flexure_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.opt_bnch_mirror_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.opt_bnch_fold_flat_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.opt_bnch_fpa_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.opt_bnch_fpe_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.opt_bnch_living_rm_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.opt_bnch_box_beam_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.opt_bnch_cover_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.field_stop_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.fpa_positive_y_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.fpa_negative_y_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.fpe_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.primary_mirror_mnt_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.primary_mirror_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.primary_mirror_baf_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ms_truss_leg_0_a_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ms_truss_leg_0_b_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ms_truss_leg_120_a_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ms_truss_leg_120_b_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ms_truss_leg_240_a_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ms_truss_leg_240_b_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.barrel_baffle_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.sun_shade_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.spider_leg_30_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.spider_leg_150_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.spider_leg_270_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.sec_mirror_mtr_rng_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.sec_mirror_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.sec_mirror_baffle_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.iea_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.focus_motor_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ie_pws_board_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_pws_board_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.mech_tlm_board_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.inst_cont_board_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   HiRISE_Power_Parameters
   description            The HiRISE_Power_Parameters class contains attributes specific to HiRISE EDRs.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.cpmm_positive_29_voltage
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_positive_29_current
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_positive_10_voltage
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_positive_10_current
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_positive_5_voltage
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_positive_5_current
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_positive_3_3_voltage
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_positive_3_3_current
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_positive_2_5_voltage
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_positive_2_5_current
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_positive_1_8_voltage
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_positive_1_8_current
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_negative_5_voltage
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.cpmm_negative_5_current
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.heater_current
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.inst_cont_fpga_pos_2_5_voltage
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.mech_tlm_fpga_pos_2_5_voltage
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.iea_positive_28_voltage
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.iea_negative_15_voltage
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.iea_positive_15_voltage
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.iea_positive_5_voltage
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   HiRISE_RDR_Parameters
   description            The HiRISE_RDR_Parameters class contains attributes specific to HiRISE RDRs.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.ccd_flag_red0
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ccd_flag_red1
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ccd_flag_red2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ccd_flag_red3
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ccd_flag_red4
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ccd_flag_red5
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ccd_flag_red6
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ccd_flag_red7
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ccd_flag_red8
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ccd_flag_red9
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ccd_flag_ir10
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ccd_flag_ir11
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ccd_flag_bg12
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ccd_flag_bg13
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_red0
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_red1
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_red2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_red3
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_red4
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_red5
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_red6
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_red7
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_red8
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_red9
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_ir10
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_ir11
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_bg12
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.binning_bg13
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_red0
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_red1
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_red2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_red3
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_red4
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_red5
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_red6
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_red7
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_red8
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_red9
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_ir10
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_ir11
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_bg12
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.tdi_bg13
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_red0
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_red1
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_red2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_red3
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_red4
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_red5
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_red6
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_red7
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_red8
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_red9
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_ir10
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_ir11
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_bg12
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.special_processing_flag_bg13
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.minimum_stretch
      minimum occurrences   0
      maximum occurrences   3
      reference type        attribute_of

      local identifier      mro.maximum_stretch
      minimum occurrences   0
      maximum occurrences   3
      reference type        attribute_of

   name                   CRISM_Hyperspectral_Data_Filter_Control_Parameters
   description            The CRISM_Hyperspectral_Data_Filter_Control_Parameters class contains attributes related to the CRISM hyperspectral data filtering application used to convert TRR3 radiance data to I/F.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.hdf_software_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.hdf_software_version_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.if_min_value
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.if_max_value
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.trace_min_value
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.trace_max_value
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.refz_median_box_width
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.refz_smooth_box_width
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.fram_stat_median_box_width
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.fram_stat_min_deviation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.fram_stat_median_conf_lvl
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.fram_stat_iqr_conf_lvl
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.rsc_ref_xy_median_width
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.rsc_ref_xy_smooth_width
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.rsc_ref_yz_median_width
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.rsc_ref_yz_smooth_width
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.rsc_ratio_xy_median_width
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.rsc_ratio_xy_smooth_width
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.rsc_res_xy_ply_order
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.rsc_res_xy_ply_extnd_width
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.log_xform_neg_clip_value
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_num_regions
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_start_channel_r1
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_start_channel_r2
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_stop_channel_r1
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_stop_channel_r2
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_confidence_level_r1
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_confidence_level_r2
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_weighting_stddev_r1
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_weighting_stddev_r2
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_kernel_size_x_r1
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_kernel_size_x_r2
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_kernel_size_y_r1
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_kernel_size_y_r2
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_kernel_size_z_r1
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_kernel_size_z_r2
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_model_order_x_r1
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_model_order_x_r2
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_model_order_y_r1
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_model_order_y_r2
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_model_order_z_r1
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ikf_model_order_z_r2
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

   name                   CRISM_Temperatures
   description            The CRISM_Temperatures class is the container for CRISM-specific temperature-related parameters.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.detector_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.optical_bench_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.spectrometer_housing_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.sphere_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.fpe_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   CRISM_Band
   description            The CRISM_Band class contains parameters describing a single band in CRISM Browse Product 3D image array or in the CRISM data cube containing refined spectral summary parameters. 
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.band_name
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.band_sequence_number
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.scaling_factor
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.value_offset
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   CRISM_Parameters
   description            The CRISM_Parameters class is the container for CRISM-specific observation parameters.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.observation_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.observation_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.observation_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.activity_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.sensor_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.instrument_pointing_mode
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.scan_mode_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.frame_rate
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.exposure_parameter
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.sampling_mode_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.wavelength_filter
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.wavelength_file_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.pixel_proc_file_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.inv_lookup_table_file_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.CRISM_Hyperspectral_Data_Filter_Control_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      mro.CRISM_Temperatures
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      mro.CRISM_Band
      minimum occurrences   0
      maximum occurrences   *
      reference type        component_of

   name                   CRISM_ATO_Parameters
   description            The CRISM_ATO_Parameters class is the container for observation parameters specific to the CRISM ATO (Along-Track Oversampled) reprocessing project.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.ato.min_line
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ato.max_line
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ato.min_sample
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.ato.max_sample
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   SHARAD_Observation_Parameters
   description             The SHARAD_Observation_Parameters class provides parameters for SHARAD radar observations. 
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.synthetic_aperture_duration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.multilook_doppler_bandwidth
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.number_of_looks
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.chirp_frequency_envelope
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.range_compression_window
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.azimuth_processing_window
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Array_Sampled
   description             The Array_Sampled class class provides parameters for a uniformly sampled array. 
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.name
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.array_interval
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.array_unit
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.array_first_value
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.array_last_value
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.array_scale
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

   name                   SHARAD_Parameters
   description            The SHARAD_Parameters class contains attributes specific to SHARAD data.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.SHARAD_Observation_Parameters
      minimum occurrences   0
      maximum occurrences   *
      reference type        component_of

      local identifier      mro.Array_Sampled
      minimum occurrences   0
      maximum occurrences   *
      reference type        component_of

   name                   MRO_Parameters
   description            The MRO_Parameters class is the container for mission-specific metadata elements.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mro.product_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.product_version_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.release_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.observation_rationale
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.orbit_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.mission_phase_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.spacecraft_clock_count_partition
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.spacecraft_clock_start_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.spacecraft_clock_stop_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.producer_institution_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.line_prefix_bytes
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.line_suffix_bytes
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mro.HiRISE_Time_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      mro.HiRISE_Instrument_Setting_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      mro.HiRISE_Temperature_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      mro.HiRISE_Power_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      mro.HiRISE_RDR_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      mro.CRISM_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      mro.SHARAD_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      mro.CRISM_ATO_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

End of Report
