PDS4 Local Data Dictionary Processing Report

Configuration:
   LDDTool Version        16.1.3
   LDD Version Id:        1.3.3.0
   LDD Label Version Id:  1.24
   LDD Discipline (T/F):  true
   LDD Namespace URL:     http://pds.nasa.gov/pds4/
   LDD URN Prefix:        urn:nasa:pds:
   Time                   Thu Sep 03 21:32:28 UTC 2026
   Common Schema          [PDS4_PDS_1I00.xsd]
   Common Schematron      [PDS4_PDS_1I00.sch]
   IM Version Id:         1.18.0.0
   IM Namespace Id:       pds
   IM Label Version Id:   1.24
   IM Object Model        [UpperModel.pont]
   IM Data Dictionary     [dd11179.pins]
   IM Glossary            [Glossary.pins]
   IM Document Spec       [DMDocument.pins]

Parameters:
   Input File             [/home/runner/work/ldd-msn/ldd-msn/src/PDS4_MSN_IngestLDD.xml]
   PDS Processing         true
   LDD Processing         true
   Discipline LDD         true
   Mission LDD            false
   Write Attr Elements    false
   Merge with Master      false

Summary:
   Classes                5
   Attributes             36
   Associations           41
   Error messages         0
   Warning messages       0
   Information messages   0

Detailed validation messages

Parsed Input - Header:
   LDD Name               Mission Information Commons
   LDD Version            1.3.3.0
   Full Name              Trent Hare
   Steward                img
   Namespace Id           msn
   Comment                
      ## CHANGE LOG ##
      1.0.0.0
      - Initial version
      
      1.1.0.0
      - Upgraded to v1B00 of the IM.
      - Re-classified this dictionary as a Discipline Dictionary, instead of Mission Dictionary.
      - Renamed Orbital_Mission_Information to Orbital_Mission, Surface_Mission_Information to Surface_Mission
      
      1.2.0.0
      - Upgraded to v1D00 of the IM.
      - Add instrument_clock_start and allow helicopter use case.
      - Add instrument_start_time. This is instrument_clock_start converted to UTC.
      - Updated the definition for start_sol_number to allow a primary sol to be 
        defined for mosaic products inplace of the actual starting sol value.
       
      1.3.0.0
      - Upgraded to v1E00 of the IM
      - Add year_number, year_number_reference attributes to Surface_Mission
      - Added Observation_Context class and attrbitues active_flight_computer, active_flight_imu under Mission_Information

      1.3.0.2
      - add instrument_clock_stop and instrument_stop_time
      - mission_phase_name and mission_phase_identifier to unbounded (multi)

     1.3.0.3
     - add ephemeris_start_time and ephemeris_stop_time to have available at the mission level.
         We do understand et_start and et_stop are also available from the nucspec dictionary but
         this is required by THEMIS which is not a nucspec instrument.

     1.3.1.0
     - add orbit_identifier to Orbital_Mission class.
     
     1.3.2.0
     - Add Observation_Description class

     1.3.3.0
      - Add flight_day_number and internal_id

    
   Last Modification Time 2026-09-03T23:00:01Z
   PDS4 Merge Flag        false

Parsed Input - Attributes:

   name                   mission_phase_name
   version                1.18
   value data type        ASCII_Short_String_Preserved
   description            The mission_phase_name identifies a time period within the mission.
   nillable               true

   name                   mission_phase_identifier
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The mission_phase_identifier attribute provides an identifier for a mission phase.
   nillable               true

   name                   release_number
   version                1.18
   value data type        ASCII_Integer
   description            Release_number is the number of a scheduled release of data from the provider to PDS. The first data release is typically Release 1. The release_number for a given product is always the first release in which it appears, and does not change if the product is revised later.
   nillable               true
   minimum value          1

   name                   product_type_name
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The product_type_name identifies a group of data products within a collection that have some property in common, such as processing level, resolution, or instrument-specific setting. 
   nillable               true

   name                   spacecraft_clock_start
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_start is the value of the spacecraft clock at the beginning of the observation.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   spacecraft_clock_stop
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_stop is the value of the spacecraft clock at the end of the observation. spacecraft_clock_stop should only be used if there's also a spacecraft_clock_start value.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   spacecraft_clock_partition
   version                1.18
   value data type        ASCII_Integer
   description            The spacecraft_clock_partition provides the clock partition active for the spacecraft_clock attribute.

   name                   instrument_clock_start
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The value of the clock returned by the instrument at the beginning of the observation. This may differ from the spacecraft clock due to several factors such as clock drift, or differences in definition of start time (for example, spacecraft clock might be when an image was commanded, but instrument clock might be after autoexpoure or autofocus processes), or differences in the time epoch between the instrument and the main spacecraft. 
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   instrument_clock_stop
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The value of the clock returned by the instrument at the end of the observation. This may differ from the spacecraft clock due to several factors such as clock drift, or differences in definition of stop time, or differences in the time epoch between the instrument and the main spacecraft. 
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   instrument_start_time
   version                1.18
   value data type        ASCII_Date_Time_YMD_UTC
   description            This is instrument_clock_start converted to UTC
   nillable               true

   name                   instrument_stop_time
   version                1.18
   value data type        ASCII_Date_Time_YMD_UTC
   description            This is instrument_clock_stop converted to UTC
   nillable               true

   name                   internal_id
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            Indentifier for this data used internally to the data provider team. Intended to help connect the data to mission documentation.

   name                   ephemeris_start_time
   version                1.18
   value data type        ASCII_Real
   description             The time of data acquisition of the leading edge of the detector array. Value given in spacecraft event time (SCET), ET format. 
   nillable               true
   unit of measure type   Units_of_Time

   name                   ephemeris_stop_time
   version                1.18
   value data type        ASCII_Real
   description            The time of the end of data acquisition. This is often calculated from the start time and image duration. Value given in spacecraft event time (SCET), ET format. 
   nillable               true
   unit of measure type   Units_of_Time

   name                   flight_day_number
   version                1.18
   value data type        ASCII_Integer
   description            Specifies the flight day number of this mission, since the mission-defined starting point (typically blaunch). 
   nillable               true

   name                   start_orbit_number
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The start_orbit_number attribute provides the first in a series of numbers that represent a set of orbital revolutions of one body around another.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   stop_orbit_number
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            The stop_orbit_number attribute provides the last in a series of numbers that represent s set of orbital revolutions of one body around another.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   orbit_identifier
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            Missions such as Cassini, JUNO and MRO, include an attribute orbit identifier whihch is more grainular then mission phase. This can be skipped or has been set to N/A for cruise images. 
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   start_sol_number
   version                1.18
   value data type        ASCII_Integer
   description            The start_sol_number is the number of the Mars day on which an observation began. Landing day is Sol 0. For multi-sol observations, such as mosaics, if start_sol_number is given but stop_sol_number is not, the start_sol_number may instead be interpreted as the primary, or most important, sol for this observation.
   nillable               true
   minimum value          0

   name                   stop_sol_number
   version                1.18
   value data type        ASCII_Integer
   description            The stop_sol_number is the number of the Mars day on which an observation ended. Landing day is Sol 0. The stop_sol_number should only be used if there's also a start_sol_number.
   nillable               true
   minimum value          0

   name                   start_local_mean_solar_time
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            start_local_mean_solar_time is the local mean solar time, as defined in the main PDS4 data dictionary.
   minimum characters     8
   maximum characters     255

   name                   stop_local_mean_solar_time
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            stop_local_mean_solar_time is the local mean solar time, as defined in the main PDS4 data dictionary.
   minimum characters     8
   maximum characters     255

   name                   start_local_true_solar_time
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            start_local_true_solar_time is the local true solar time, as defined in the main PDS4 data dictionary.
   minimum characters     8
   maximum characters     255

   name                   stop_local_true_solar_time
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            stop_local_true_solar_time is the local true solar time, as defined in the main PDS4 data dictionary.
   minimum characters     8
   maximum characters     255

   name                   solar_longitude
   version                1.18
   value data type        ASCII_Real
   description            solar_longitude is the solar longitude, as defined in the main PDS4 data dictionary.
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   start_local_mean_solar_time_sol
   version                1.18
   value data type        ASCII_Integer
   description            The start_local_mean_solar_time_sol element specifies the number of solar days elapsed since a reference day (e.g. the day on which a landing vehicle set down) for local mean solar time (LMST). Days are measured in rotations of the planet in question from midnight to midnight. The reference day is '0', as Landing day is Sol 0. If before Landing day, then value will be less than or equal to '0'and can be negative.

   name                   stop_local_mean_solar_time_sol
   version                1.18
   value data type        ASCII_Integer
   description            The stop_local_mean_solar_time_sol element specifies the number of solar days elapsed since a reference day (e.g. the day on which a landing vehicle set down) for local mean solar time (LMST). Days are measured in rotations of the planet in question from midnight to midnight. The reference day is '0', as Landing day is Sol 0. If before Landing day, then value will be less than or equal to '0'and can be negative. The stop_local_mean_solar_time_sol should only be used if there's also a start_local_mean_solar_time_sol.

   name                   start_local_true_solar_time_sol
   version                1.18
   value data type        ASCII_Integer
   description            The start_local_true_solar_time_sol element specifies the number of solar days elapsed since a reference day (e.g. the day on which a landing vehicle set down) for local true solar time (LTST). Days are measured in rotations of the planet in question from midnight to midnight. The reference day is '0', as Landing day is Sol 0. If before Landing day, then value will be less than or equal to '0'and can be negative.

   name                   stop_local_true_solar_time_sol
   version                1.18
   value data type        ASCII_Integer
   description            The stop_local_true_solar_time_sol element specifies the number of solar days elapsed since a reference day (e.g. the day on which a landing vehicle set down) for local true solar time (LTST). Days are measured in rotations of the planet in question from midnight to midnight. The reference day is '0', as Landing day is Sol 0. If before Landing day, then value will be less than or equal to '0'and can be negative. The stop_local_true_solar_time_sol should only be used if there is also a start_local_true_solar_time_sol.

   name                   year_number
   version                1.18
   value data type        ASCII_Integer
   description            Identifies the year of the observation, using the definition for year specified in year_number_reference.

   name                   year_number_reference
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            Identifies the system used to measure year_number. Current values include: Mars Year: Mars year as defined by Piqueaux et al (2015), extending Clancy et al (2000). Mars Year 1 started on April 11, 1955 at Ls (areocentric solar longitude) = 0, with subsequent years starting at Ls=0. Reference: https://doi.org/10.1016/j.icarus.2014.12.014
   minimum characters     1
   maximum characters     255

   name                   active_flight_computer
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            Identifies which of potentially several flight computers were used for this observation.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   active_flight_imu
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description            Identifies which of potentially several inertial measurement units (IMUs) were used for this observation.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   observation_id
   version                1.18
   value data type        ASCII_Short_String_Collapsed
   description             Uniquely identifies this observation within the context of the mission. Products with the same observation_id should be part of the same observation. 
   minimum characters     1
   maximum characters     255

   name                   observation_start_date_time
   version                1.18
   value data type        ASCII_Date_Time_YMD_UTC
   description             Identifies the start date and time for the observation as a whole (not just this individual product). 

   name                   observation_stop_date_time
   version                1.18
   value data type        ASCII_Date_Time_YMD_UTC
   description             Identifies the stop date and time for the observation as a whole (not just this individual product). 

Parsed Input - Classes:

   name                   Mission_Information
   description            The Mission_Information class provides information about a mission.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      msn:mission_phase_name
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      msn:mission_phase_identifier
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      msn:release_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:product_type_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:spacecraft_clock_start
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:spacecraft_clock_stop
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:spacecraft_clock_partition
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:instrument_clock_start
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:instrument_clock_stop
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:instrument_start_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:instrument_stop_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:ephemeris_start_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:ephemeris_stop_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:flight_day_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:internal_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:Orbital_Mission
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      msn:Surface_Mission
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      msn:Observation_Context
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      msn:Observation_Description
      minimum occurrences   0
      maximum occurrences   *
      reference type        component_of

   name                   Orbital_Mission
   description            The Orbital_Mission class provides information about an orbital mission.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      msn:start_orbit_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:stop_orbit_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:orbit_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Surface_Mission
   description            The Surface_Mission class provides information about a surface mission.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      msn:start_sol_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:stop_sol_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:start_local_mean_solar_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:stop_local_mean_solar_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:start_local_mean_solar_time_sol
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:stop_local_mean_solar_time_sol
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:start_local_true_solar_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:stop_local_true_solar_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:start_local_true_solar_time_sol
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:stop_local_true_solar_time_sol
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:solar_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:year_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:year_number_reference
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Observation_Context
   description            Describes the vehicle context at the time the observation was taken.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      msn:active_flight_computer
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:active_flight_imu
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Observation_Description
   description             Describes the observation, which may consist of a set of related products (for example, different spectral filters on the same target, or different frames of a movie or mosaic). Products that are part of the same observation should have the same observation_id. Note that a product can be part of multiple Observation_Descriptions. 
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.description
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:observation_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:observation_start_date_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      msn:observation_stop_date_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

End of Report
