                            1-01 VERSION DATE:  980601

                 Chapter 1 - Introduction

                         Contents

                         ________

       Sub-Section                                      Page

1.0    Contents  .....................................    1

1.1    Introduction  .................................    2

                                 1-02

Introduction

____________

     From May 22, 1996 through June 01, 1996 the Galileo spacecraft
will load and test the new Phase 2 CDS software.  This time period
is known as the In-Flight Load (IFL).  NIMS will also reload its own
Phase 2 software at this time.  This handbook is provided to the
NIMS Team as a guide to the IFL.

     During this time period, NIMS will take advantage of the new
Phase 2 capabilities of both NIMS and CDS to perform a series of
Optical Calibrations (OPCALs) and return the data using the new
real-time capabilities of the spacecraft.  This series of OPCALs
will give the NIMS Team an indication of how well the new Phase 2
software (both NIMS and CDS) is performing on the spacecraft.  It
will also give an indication of the health of the NIMS instrument
as NIMS has not been used since the SL9 Encounter back in July of
1994, nearly two years ago.

     The NIMS Phase 2 software has some new features, including
wavelength editing and mirror blocking, which will be tested at this
time.  Wavelength editing will be used to select only detectors 1 and
2 for all Long Map grating positions.  Mirror blocking will be used to
select only mirror positions 8-11 (of 0-19).  The data will then be
returned using the new real-time capabilities of the spacecraft.

     The new Galileo Ground Data System (GDS) and AMMOS will also be
tested in preparation for Orbital Operations as well as the MIPS real
time data processing.  This will test the entire ground path from DSN
Station to UDR to Tube.