PDS4 Local Data Dictionary Processing Report

Configuration:
   LDDTool Version        15.3.0
   LDD Version Id:        1.1.0.0
   LDD Label Version Id:  1.0
   LDD Discipline (T/F):  false
   LDD Namespace URL:     http://pds.nasa.gov/pds4/
   LDD URN Prefix:        urn:nasa:pds:
   Time                   Fri May 23 14:52:56 UTC 2025
   Common Schema          [PDS4_PDS_1N00.xsd]
   Common Schematron      [PDS4_PDS_1N00.sch]
   IM Version Id:         1.23.0.0
   IM Namespace Id:       pds
   IM Label Version Id:   1.0
   IM Object Model        [UpperModel.pont]
   IM Data Dictionary     [dd11179.pins]
   IM Glossary            [Glossary.pins]
   IM Document Spec       [DMDocument.pins]

Parameters:
   Input File             [/home/runner/work/ldd-mgn/ldd-mgn/src/PDS4_MGN_IngestLDD.xml]
   PDS Processing         true
   LDD Processing         true
   Discipline LDD         false
   Mission LDD            true
   Write Attr Elements    false
   Merge with Master      false

Summary:
   Classes                1
   Attributes             17
   Associations           17
   Error messages         0
   Warning messages       0
   Information messages   0

Detailed validation messages

Parsed Input - Header:
   LDD Name               MGN
   LDD Version            1.1.0.0
   Full Name              Jenn Ward
   Steward                geo
   Namespace Id           mgn
   Comment                
        The MGN dictionary contains classes that describe aspects of the 
        Magellan mission and related instruments.
        
        MGN version 1.1.0.0
        PDS Build 1.22.0.0 (1M00)
        LDDTool version 15.1.0
        
        Created with lddtool -plJ -V 1M00 PDS4_MGN_IngestLDD.xml
    
   Last Modification Time 2024-12-04
   PDS4 Merge Flag        false

Parsed Input - Attributes:

   name                   band_name
   version                1.23
   value data type        ASCII_Short_String_Collapsed
   description             The name of the radio band in which the signal was received. 

   name                   dsn_station_number
   version                1.23
   value data type        ASCII_NonNegative_Integer
   description             The number of the DSN antenna used to collect the data. 
   minimum value          0
   maximum value          99

   name                   mapping_cycle
   version                1.23
   value data type        ASCII_NonNegative_Integer
   description            The mapping cycle in which the data were acquired. Should be 1 to 6. 
   minimum value          1
   maximum value          6

   name                   mission_phase_name
   version                1.23
   value data type        ASCII_Short_String_Collapsed
   description             The mission_phase_name attribute provides the mission-defined name of a time period within the mission. 

   name                   organization_id
   version                1.23
   value data type        ASCII_Short_String_Collapsed
   description             The organization that produced the data. 

   name                   orbit_number
   version                1.23
   value data type        ASCII_NonNegative_Integer
   description            The orbit_number attribute identifies the number of the orbital revolution around a target body. 
   minimum value          1
   maximum value          20000

   name                   original_pds_volume_id
   version                1.23
   value data type        ASCII_Short_String_Collapsed
   description            The original PDS volume_id of where the Magellan data are located. 

   name                   producer_institution_name
   version                1.23
   value data type        ASCII_Short_String_Collapsed
   description            The producer_institution_name attribute identifies a university, research center, NASA center, or other institution associated with the production of a data product. 

   name                   product_type
   version                1.23
   value data type        ASCII_Short_String_Collapsed
   description            The product_type attribute indicates the type of data for an individual data product. The values are based on the values used by the Magellan project for their delivery to PDS.

   name                   product_version_id
   version                1.23
   value data type        ASCII_Short_String_Collapsed
   description            The product_version_id attribute identifies the version of an individual data product. 

   name                   radar_look_direction
   version                1.23
   value data type        ASCII_Short_String_Collapsed
   description             The radar_look_direction attribute provides the direction the radar antenna was pointing relative to the spacecraft ground track along a given orbit. Most cases were Left or Right. Stereo indicates left looking with an incidence angle for stereo measurements. Maxwell is a special case for observing the Maxwell feature. 

   name                   received_polarization_type
   version                1.23
   value data type        ASCII_Short_String_Collapsed
   description             The radio polarization of the receiving antenna and feed. 

   name                   spacecraft_clock_count_partition
   version                1.23
   value data type        ASCII_NonNegative_Integer
   description            The spacecraft_clock_count_partition attribute indicates the clock partition active for the spacecraft_clock_start_count and spacecraft_clock_stop_count attributes. 

   name                   spacecraft_clock_start_count
   version                1.23
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_start_count attribute provides the value of the spacecraft clock at the beginning of a time period of interest. 
   nillable               true

   name                   spacecraft_clock_stop_count
   version                1.23
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_stop_count attribute provides the value of the spacecraft clock at the end of a time period of interest. 
   nillable               true

   name                   start_orbit_number
   version                1.23
   value data type        ASCII_NonNegative_Integer
   description            Provides the the lowest revolution orbit number that contributed data to a given data product. 
   minimum value          1
   maximum value          20000

   name                   stop_orbit_number
   version                1.23
   value data type        ASCII_NonNegative_Integer
   description            Provides the the highest revolution orbit number that contributed data to a given data product. 
   minimum value          1
   maximum value          20000

Parsed Input - Classes:

   name                   Magellan_Parameters
   description            The Magellan_Parameters class is the container for mission-specific metadata elements.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      mgn:product_type
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:product_version_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:mapping_cycle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:orbit_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:start_orbit_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:stop_orbit_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:mission_phase_name
      minimum occurrences   0
      maximum occurrences   unbounded
      reference type        attribute_of

      local identifier      mgn:radar_look_direction
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:spacecraft_clock_count_partition
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:spacecraft_clock_start_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:spacecraft_clock_stop_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:band_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:received_polarization_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:dsn_station_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:organization_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:producer_institution_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mgn:original_pds_volume_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

End of Report
