PDS4 Local Data Dictionary Processing Report

Configuration:
   LDDTool Version        16.1.3
   LDD Version Id:        1.0.0.0
   LDD Label Version Id:  1.0
   LDD Discipline (T/F):  false
   LDD Namespace URL:     http://pds.nasa.gov/pds4/
   LDD URN Prefix:        urn:nasa:pds:
   Time                   Fri Jun 19 17:42:49 UTC 2026
   Common Schema          [PDS4_PDS_1O00.xsd]
   Common Schematron      [PDS4_PDS_1O00.sch]
   IM Version Id:         1.24.0.0
   IM Namespace Id:       pds
   IM Label Version Id:   1.0
   IM Object Model        [UpperModel.pont]
   IM Data Dictionary     [dd11179.pins]
   IM Glossary            [Glossary.pins]
   IM Document Spec       [DMDocument.pins]

Parameters:
   Input File             [/home/runner/work/ldd-phoenix/ldd-phoenix/src/PDS4_PHOENIX_IngestLDD.xml]
   PDS Processing         true
   LDD Processing         true
   Discipline LDD         false
   Mission LDD            true
   Write Attr Elements    false
   Merge with Master      false

Summary:
   Classes                2
   Attributes             12
   Associations           13
   Error messages         0
   Warning messages       0
   Information messages   0

Detailed validation messages

Parsed Input - Header:
   LDD Name               Mars Phoenix Mission Dictionary
   LDD Version            1.0.0.0
   Full Name              Jennifer Ward
   Steward                geo
   Namespace Id           phoenix
   Comment                
        The Mars Phoenix mission dictionary contains classes and attributes specific to the Mars Phoenix mission and its instruments.
        
        Phoenix version 1.0.0.0
        PDS Build 1.24.0.0 (1O00)
        LDDTool version 15.3.0
        
        Created with lddtool -plJ PDS4_PHOENIX_IngestLDD.xml
        
        Change Log
        6/11/2026 GEO/JGW Initial version
        
    
   Last Modification Time 2026-06-11Z
   PDS4 Merge Flag        false

Parsed Input - Attributes:

   name                   instument_mode_id
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The instument_mode_id attribute identifies an instrument-dependent designation of operating mode.

   name                   local_true_solar_time
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The local_true_solar_time attribute is the local true solar time, as defined in the main PDS4 data dictionary, at the beginning of an observation.

   name                   mission_phase_name
   version                1.24
   value data type        ASCII_Short_String_Preserved
   description            The mission_phase_name identifies a time period within the mission.

   name                   ops_token
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The ops_token is a code associated with a Phoenix data product that provides information about the command sequence that caused the product to be acquired. The value is a 32-bit unsigned hexadecimal integer expressed in a PDS label as 16#AAAAPCCC#, where: - AAAA is the campaign ID assigned by the sequence planning team, - P is a 4-bit payload ID reserved for use by each instrument team, as defined by the team, and - CCC is the command sequence number, which is set to zero for each new campaign and automatically incremented with each command. The combination of ops_token and sol number should uniquely identify a Phoenix data product.

   name                   ops_token_activity
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            ops_token_activity is the 16-bit activity code (campaign id) from the ops_token, represented as a 4-digit Hex value.

   name                   ops_token_command
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            ops_token_command is the 12-bit command sequence number of the ops token, represented as a 3-digit Hex value.

   name                   ops_token_payload
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            ops_token_payload is the 4-bit payload id value of the ops token, represented as a single Hex digit.

   name                   product_type
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The product_type attribute identifies a group of data products within a collection that have some property in common. 

   name                   product_version_id
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The product_version_id attribute identifies the version of an individual data product. 

   name                   sol_number
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The sol_number attibute is the number of the Mars day on which an observation was acquired. Landing day is Sol 0. 

   name                   spacecraft_clock_start
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_start attribute provides the value of the spacecraft clock at the beginning of a time period of interest. 

   name                   spacecraft_clock_stop
   version                1.24
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_stop attribute provides the value of the spacecraft clock at the end of a time period of interest. 

Parsed Input - Classes:

   name                   Observation_Information
   description            The Observation_Information class provides information about a science observation.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      phoenix.mission_phase_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      phoenix.product_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      phoenix.product_version_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      phoenix.spacecraft_clock_start
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      phoenix.spacecraft_clock_stop
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      phoenix.local_true_solar_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      phoenix.sol_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      phoenix.ops_token
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      phoenix.ops_token_activity
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      phoenix.ops_token_payload
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      phoenix.ops_token_command
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      phoenix.instrument_mode_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Phoenix_Parameters
   description            The Phoenix_Parameters class is a superclass containing all Phoenix mission classes.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      phoenix.Observation_Information
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

End of Report
